Files in the folder

1. Sharp_MP_Field_3_Readme_B.txt		the file you are reading
2. Sharp_MP_Field_3_B.jvt			bitstream file
3. Sharp_MP_Field_3_rec_B.yuv		reconstructed YUV file
4. Sharp_MP_Field_3_trace_dec_B.txt	decoder trace file, generated by JM6.2 decoder

Encoder configuration:
Stream Name:             Sharp_MP_Field_3_B  
Stream Source:           Sharp
Video Sequence:          Bus  
Video Resolution:        720x480  
Video Frames:            15 
Frame/Field Coding:      Field  
Entropy Coding:          CAVLC  
Slice Types:             IP  
Slices per Picture:      1  
Conformance Point:       JVT-G050  
POC Type:                1  
Number Ref Frames:       5  
IDR:                     First frame  
Ref Pic List Reorder:    No  
Adapt Ref Pic Mark:      Off  
Constrained Intra Pred:  Off  
Weighted Pred (P):       Off  
Weighted Bipred (B):     Off  
Direct Prediction:       Yes  
Direct 8x8 Inference:    Yes
Loop Filter:             Off  
SEI:                     No  
VUI:                     No  
Number Slice Groups:     1
Long-term Ref Frames:    No
MMCO:                    No
Arbitrary Slice Order:   No
Redundant Slices:        No
