Files in the folder

1. Sharp_MP_PAFF_1r2_Readme.txt		the file you are reading
2. Sharp_MP_PAFF_1r2.jvt			bitstream file
3. Sharp_MP_PAFF_1r2_rec.yuv		reconstructed YUV file
4. Sharp_MP_PAFF_1r2_trace_dec.txt	decoder trace file, generated by JM6.2 decoder

Encoder configuration:
Stream Name:             Sharp_MP_PAFF_1
Stream Source:           Sharp
Video Sequence:          Bus  
Video Resolution:        720x480  
Video Frames:            15 
Frame/Field Coding:      Picture-level Adaptive-Frame-Field Coding
Entropy Coding:          CAVLC  
Slice Types:             IP  
Slices per Picture:      1  
Conformance Point:       JVT-G050  
POC Type:                1  
Number Ref Frames:       5  
IDR:                     First frame  
Ref Pic List Reorder:    No  
Adapt Ref Pic Mark:      Off  
Constrained Intra Pred:  Off  
Weighted Pred (P):       Off  
Weighted Bipred (B):     Off  
Direct Prediction:       Spatial  
Direct 8x8 Inference:    Yes
Loop Filter:             Off  
SEI:                     No  
VUI:                     No  
Number Slice Groups:     1
Long-term Ref Frames:    No
MMCO:                    No
Arbitrary Slice Order:   No
Redundant Slices:        No
