ENTP_A_Qualcomm_1

Specification version: HM13.0

Category: Entry Point
Replacement for ENTP_X_LG_X conformance test bitstreams

Specification:
- 1080p60 
- 24 frames 
- Intra-Main configuration
- One slice per picture
- Four tiles per picture
	* num_tiles_columns_minus1 = 1
	* num_tiles_rows_minus1 = 1
	* uniform_spacing_idc = 1
- MD5 checksum is included in the bitstream
NOTE: There are some tiles in POC 4 that contains emulation prevention bytes

Purpose: Test entry point signalling in slice header when tile is used and when emulation prevention bytes occur in substream(s)
