OPFLAG_B_Qualcomm_1

Specification version: HM13.0

Category: Picture output

Specification:
- 480p60 
- 100 frames 
- All intra configuration
- One slice per picture
- Output flag present indicidation in PPS is set
- Picture with POC 39 and 73 are set to be not for output.
- MD5 checksum is included in the bitstream

Purpose: Test picture output flag indication
