|  |  |  |
| --- | --- | --- |
| **Radiocommunication Bureau (BR)** | | |
| Circular Letter  **CR/391** | | 29 February 2016 |
|  | | |
|  | | |
| **To Administrations of Member States of the ITU** | | |
|  | | |
|  | | |
| Subject: | **Notification of frequency assignments to IMT stations for recording in the Master Register** | |
|  |
|  |
|  | | |

The World Radiocommunication Conference, Geneva, 2015 (WRC-15) took a number of decisions on the revision of the table of frequency allocations (Article 5 of the Radio Regulations), including the identification for the implementation of IMT (International Mobile Telecommunications) in several frequency bands between 470 MHz and 4 990 MHz.

This identification for IMT has been associated with regulatory and technical conditions imposed on this particular use of the mobile service. Examples of identification for IMT and the associated conditions, such as operation on a non-interference basis, power flux density limits and the obligation to obtain agreement under **No.9.21**, can be found, inter alia, in Nos. **5.295** (**5.idR2a**), **5.341A** (**5.R1a**), **5.346A** (**5.R3h**).

In order to distinguish the frequency assignments to IMT stations from other stations in the mobile service, and enable the examination of the conditions associated with IMT, the Bureau has introduced a new symbol for Nature of Service in Table 7.1 of the Preface to BRIFIC (terrestrial services), as follows: **IM** – IMT station in the mobile service.

Administrations are therefore invited to use this symbol when notifying frequency assignments to IMT stations for their recording in the Master Register.

François Rancy

Director

Distribution:

– Administrations of Member States of the ITU

– Members of the Radio Regulations Board