**Chad (country code +235)**

Communication of 25.XI.2015:

The *Autorité de Régulation des Communications Electroniques et des Postes*, N'Djamena, announces the following update in the national numbering plan of Chad.

General information:

Country Code: 235

International Prefix: 00

National Prefix: --

Length of national (significant) number
(excluding national prefix): minimum 8 digits

 maximum 8 digits

Universal Time Coordinated/Summer Time: UTC +1

Description of introduction of new resource for national numbering plan for country code 235:

| (1) | (2) | (3) | (4) |
| --- | --- | --- | --- |
| *NDC (National Destination Code) or leading digits of N(S)N (National (Significant) Number)* | *N(S)N Number length* | *Usage ofITU-T E.164 number* | *Time and date of introduction* |
| *Maximum length* | *Minimum length* |
| 65000000 – 65999999  | 8 | 8 | Non-geographic number – mobile telephony service – assigned to AIRTEL-TCHAD | 14.I.2015 |

Contact:

Mr. Hisseine Hassane

Autorité de Régulation des Communications Electroniques et des Postes

Avenue du Général Daoud Soumaïne

B.P. 5808

N'DJAMENA

Chad

Tel: +235 66 25 60 70

Fax: +235 22 52 15 17

E-mail: contact@arcep.td; hisseinhas@yahoo.fr

Communication of 22.II.2010:

The *Office Tchadien de Régulation des Télécommunications (OTRT),* N'Djamena, announces that the current seven- (7) digit National Numbering Plan (NNP) of Chad will migrate to a new eight- (8) digit numbering plan. The change will be introduced as from 15 March 2010 at midnight, local time.

The new structure of the Chad National Numbering Plan will be: ABPQMCDU.

In this structure, all letters can have value between 0 and 9. The first two digits (AB) or number blocks designate the service or network. The remaining six (6) digits (PQMCDU) designate the user, unless there is a particular specification.

Break-down of digit A:

| A | Service or network |
| --- | --- |
| 0 | International access, prefix for number portability (fixed and mobile) |
| 1 | Special services  |
| 2 | Fixed network services  |
| 3, 4, 5 | Reserved for future use |
| 6, 7, 9 | Mobile network services  |
| 8 | Value-added services  |

• *International access*

International access remains unchanged. International calls continue to be dialled as follows:

00 + country code + National (Significant) Number (N(S)N

• *Fixed telephony network*

As from 15 March 2010, subscriber numbers of operators of fixed telephony will be modified as follows:

| Fixed operator | Old numbers | New numbers |
| --- | --- | --- |
| Sotel Tchad (fixed) | 2 50 XX XX2 51 XX XX2 52 XX XX2 53 XX XX2 54 XX XX2 55 XX XX2 68 XX XX2 69 XX XX | 22 50 XX XX22 51 XX XX22 52 XX XX22 53 XX XX22 54 XX XX22 55 XX XX22 68 XX XX22 69 XX XX |
| Sotel Tchad (semi-fixed) "TAWALI" | 2 30 XX XX2 70 XX XX2 80 XX XX2 90 XX XX | 22 30 XX XX22 70 XX XX22 80 XX XX22 90 XX XX |
| Sotel Tchad "SALAM" | 7 XX XX XX | 77 XX XX XX |

• *Mobile telephony networks*

As from 15 March 2010, subscriber numbers of the two mobile operators will be changed as follows:

| Mobile operator | Old numbers | New numbers |
| --- | --- | --- |
| Zain | 3 0X XX XX3 1X XX XX3 2X XX XX3 3X XX XX3 4X XX XX6 0X XX XX6 1X XX XX6 2X XX XX6 3X XX XX6 4X XX XX6 5X XX XX6 6X XX XX6 7X XX XX6 8X XX XX6 9X XX XX | 63 0X XX XX63 1X XX XX63 2X XX XX63 3X XX XX63 4X XX XX66 0X XX XX66 1X XX XX66 2X XX XX66 3X XX XX66 4X XX XX66 5X XX XX66 6X XX XX66 7X XX XX66 8X XX XX66 9X XX XX |
| Millicom | 5 0X XX XX5 1X XX XX5 2X XX XX5 3X XX XX5 4X XX XX9 0X XX XX9 1X XX XX9 2X XX XX9 3X XX XX9 4X XX XX9 5X XX XX9 6X XX XX9 7X XX XX9 8X XX XX9 9X XX XX | 95 0X XX XX95 1X XX XX95 2X XX XX95 3X XX XX95 4X XX XX99 0X XX XX99 1X XX XX99 2X XX XX99 3X XX XX99 4X XX XX99 5X XX XX99 6X XX XX99 7X XX XX99 8X XX XX99 9X XX XX |

Contact:

 Office Tchadien de Régulation des Télécommunications (OTRT)
B.P. 5808
N'DJAMENA
Chad
Tel: +235 2 52 15 13 (As from 15 March 2010: +235 22 52 15 13)
Fax: +235 2 52 15 17 (As from 15 March 2010: +235 22 52 15 17)
E-mail: info@otrt.org
URL: www.otrt.org