**Djibouti (country code +253)**

Communication of 3.I.2012:

*Djibouti Télécom S.A,* Djibouti, announces that the National Numbering Plan will change to eight (8) digits for all networks and services of Djibouti Télécom, as from 1 March 2012:

Time zone (Djibouti : UTC+3)

The National Numbering Plan (NNP) will change from six (6) to to eight (8) digits according to ITU-T Recommendation E.164.

Djibouti (country code +253).

The international prefix to dial from Djibouti Republic to reach the automatic network remains « 00 ».

1. General Structure:

The new National Numbering Plan of Djibouti Republic will be a 8 digits closed plan without national prefix in the form: ABPQMCDU

2. Tables of transition

2.1 Table of transition of the Geographic numbers for the fixed services

| ZONE 1 (DJIBOUTI CITY+BALBALA+NEIGHBOURHOOD surrounding areas) | | | | |
| --- | --- | --- | --- | --- |
| *Old number (PQMCDU)* | | | *New Number (ABPQMCDU)* | |
| *Service* | *Locality* | *Current Number* | *Digits to add* | *New Number  21 PQMCDU* |
| Fixed line | Djibouti city | 25 XX XX  29 XX XX  30 XX XX  31 XX XX  32 XX XX  34 XX XX  35 XX XX  45 XX XX | 21 | 21 25 XX XX  21 29 XX XX  21 30 XX XX  21 31 XX XX  21 32 XX XX  21 34 XX XX  21 35 XX XX  21 45 XX XX |
|  | Balbala | 31 XX XX  36 XX XX  39 XX XX | 21 | 21 31 XX XX  21 36 XX XX  21 39 XX XX |
| Fixed CDMA ZTE | Djibouti city | 57 XX XX | 21 | 21 57 XX XX |
|  | Balbala | 58 XX XX | 21 | 21 58 XX XX |

| ZONE 2 (DISTRICTS)) | | | | |
| --- | --- | --- | --- | --- |
| *Old number (PQMCDU)* | | | *New Number (ABPQMCDU)* | |
| *Service* | *Locality* | *Current number* | *Digits to add* | *New Number  27 PQMCDU* |
| Fixed line | Dikhil  Arta  Tadjourah  Ali-Sabieh  Obock | 42 0X XX  42 2X XX  42 4X XX  42 6X XX  42 8X XX | 27 | 27 42 0X XX  27 42 2X XX  27 42 4X XX  27 42 6X XX  27 42 8X XX |
| Fixed CDMA HUAWEI (rural) | Arta  Tadjourah  Dikhil  Ali-Sabieh  Obock | 50 XX XX  51 XX XX  52 XX XX  53 XX XX  54 XX XX | 27 | 27 50 XX XX  27 51 XX XX  27 52 XX XX  27 53 XX XX  27 54 XX XX |

Table 2.2 Table of transition for the mobile services numbers

Operator Djibouti telecom

| *New Number (ABPQMCDU)* | | *New Number (ABPQMCDU)* | | |
| --- | --- | --- | --- | --- |
| *Service* | *Current Number* | *Digit to add* | *New Number  77 PQ MC DU* |
| Mobile GSM | 60 XX XX  61 XX XX  62 XX XX  63 XX XX  64 XX XX  65 XX XX  66 XX XX  67 XX XX  68 XX XX  69 XX XX  70 XX XX  71 XX XX  72 XX XX  73 XX XX  74 XX XX  75 XX XX  76 XX XX  77 XX XX  78 XX XX  79 XX XX  80 XX XX  81 XX XX  82 XX XX  83 XX XX  84 XX XX  85 XX XX  86 XX XX  87 XX XX  88 XX XX  89 XX XX | 77 | 77 60 XX XX  77 61 XX XX  77 62 XX XX  77 63 XX XX  77 64 XX XX  77 65 XX XX  77 66 XX XX  77 67 XX XX  77 68 XX XX  77 69 XX XX  77 70 XX XX  77 71 XX XX  77 72 XX XX  77 73 XX XX  77 74 XX XX  77 75 XX XX  77 76 XX XX  77 77 XX XX  77 78 XX XX  77 79 XX XX  77 80 XX XX  77 81 XX XX  77 82 XX XX  77 83 XX XX  77 84 XX XX  77 85 XX XX  77 86 XX XX  77 87 XX XX  77 88 XX XX  77 89 XX XX |

3. Detailed structure of the new numbering plan

3.1 Detailed structure of numbers for geographique services (2BPQMCDU)

* Zone 1 (B=1) : Djibouti city + Balbala + surrounding areas
* Zone 2 (B=7) : the 5 internal regions

| *A* | *B* | *PQMCDU* | *Type of Numbers* | *Theoretical capacity* |
| --- | --- | --- | --- | --- |
| *Service* | *Zone* | *Number by PQ* |  |  |
| 2 | 1 | PQ MC DU | Fixed geographical number Djibouti city + Balbala | 1 Million |
| 2 | 7 | PQ MC DU | Fixed geographical number for the regions | 1 Million |

2.2 Detailed structure of numbers for mobile services (2BPQMCDU)

* Operator 1 (B=7) : Djibouti Telecom

| *A* | *B* | *PQ MC DU* | *Type of Numbers* | *Theoretical capacity* |
| --- | --- | --- | --- | --- |
| *Service* | *Zone* | *Number by PQ* |  |  |
| 7 | 7 | PQ MC DU | Mobile GSM number Djibouti Telecom | 1 Million |

The numbers for technical tests for exchanges are as follows :

Fixed Service :

Locality of Balbala : Test  number: +253 21 36 00 03

District : Test  number: +253 21 42 60 08

Locality of Djibouti :  Test  number: +253 21 30 00 00, +253 21 35 00 45 et +253 21 57 00 09

Mobiles service Test  number +253 77 83 10 01 et +253 77 84 31 31

Contact:

Mr Abdallah Mohamed-Abdallah

Responsable du Centre de Tests

Djibouti Télécom S.A.

3, Boulevard G. Pompidou

B.P. 2105

DJIBOUTI

Djibouti

Tel : +253 83 10 01 (As from 1 March 2012, Tel ; +253 77 83 10 01)

Fax : +253 35 57 57 (As from 1 March 2012, Fax : +253 21 35 57 57)

E-mail : abdallah\_mohamed@intnet.dj