**Senegal (country code +221)**

Communication of 3.X.2023:

The *Autorité de Régulation des Télécommunications et des Postes (ARTP)*, Dakar, announces the following update of the national numbering plan (NNP) for telephony in Senegal.

*Description of introduction of new resource   
for national numbering plan for country code 221:*

| *National destination code (NDC) or leading digits of national (significant) number (N(S)N)* | *N(S)N number length* | | *Usage of  ITU-T E.164 number* | *Time and date of introduction* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| 7011 | 9 | 9 | Non-geographic number –  Mobile telephone service for licensed mobile network operator EXPRESSO SENEGAL | 23 December 2022 |
| 7037 |
| 7042 |
| 7053 |
| 7066 |
| 7865 | 9 | 9 | Non-geographic number –  Mobile telephone service for licensed mobile network operator SONATEL SA | 16 June 2023 |
| 7866 |
| 7867 |
| 7868 |
| 7869 |
| 7870 |
| 7693 | 9 | 9 | Non-geographic number –  Mobile telephone service for licensed mobile network operator SAGA AFRICA HOLDINGS LIMITED | 16 August 2023 |
| 7695 |
| 7696 |
| 7697 |
| 7698 |
| 7699 |
| 7510 | 9 | 9 | Non-geographic number –  Mobile telephone service for mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 1 July 2022 |
| 7565 | 1 June 2023 |

Contact:

Mr Abdourahmane NIANG and Ms Mously Mbacké DIENE

Autorité de Régulation des Télécommunications et des Postes (ARTP)

B.P. 14130

DAKAR PEYTAVIN

Senegal

Tel: +221 33 869 0369 / direct: +221 33 869 03 93

Fax: +221 33 869 0370

E-mail: abdourahmane.niang@artp.sn; mously.diene@artp.sn

URL: www.artp.sn

Communication of 6.IX.2022:

The *Autorité de Régulation des Télécommunications et des Postes (ARTP)*, Dakar, announces the following update of the national numbering plan (NNP) for telephony in Senegal.

*Description of introduction of new resource   
for national numbering plan for country code 221:*

| *National destination code (NDC) or leading digits of national (significant) number (N(S)N)* | *N(S)N number length* | | *Usage of  ITU-T E.164 number* | *Time and date of introduction* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| 7510 | 9 | 9 | Non-geographic number –  Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 1 July 2022 |

*Presentation of national numbering plan   
for country code 221:*

a) Overview:

The minimum number length (excluding the country code) is **9** digits.

The maximum number length (excluding the country code) is **9** digits.

b) Link to the national database (or any applicable list) with assigned ITU-T E.164 numbers within the national numbering plan (if any): n/a

c) Link to the real-time database reflecting ported ITU-T E.164 numbers (if any):n/a

d) Detail of numbering plan:

| *National destination code (NDC) or leading digits of national (significant) number (N(S)N)* | *N(S)N number length* | | *Usage of  ITU-T E.164 number* | *Additional information* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| 30 | 9 | 9 | Non-geographic number – Fixed telephony service | Operator Expresso Sénégal |
| 32 | 9 | 9 | Non-geographic number – Fixed telephony service | Operator FREE Sénégal |
| 338 | 9 | 9 | Geographic number –  Fixed telephony service | Operator SONATEL (Orange), region of Dakar |
| 339 | 9 | 9 | Geographic number –  Fixed telephony service | Operator SONATEL (Orange), other regions |
| 36 | 9 | 9 | Non-geographic number –  Fixed telephony service | Operator CSU SA (HAYO) |
| 39 | 9 | 9 | Non-geographic number –  Fixed telephony service | ADIE |
| 70 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator Expresso Sénégal |
| 72 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator CSU SA (HAYO) |
| 75 | 9 | 9 | Non-geographic number – Mobile telephone service | Dedicated for mobile virtual network operators (MVNO) |
| 76 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator FREE Sénégal |
| 77 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator SONATEL (Orange) |
| 78 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator SONATEL (Orange) |
| 79 | 9 | 9 | Non-geographic number – Mobile telephone service | ADIE |
| 93 | 9 | 9 | Non-geographic number – Fixed Voice over Internet Protocol (VoIP) telephony service | Dedicated for internet service providers (*Fournisseurs d’accès à internet (FAI)*) |

Contact:

Ms Mously Mbacké DIENE and Mr Mamadou Ousmane FAYE

Autorité de Régulation des Télécommunications et des Postes (ARTP)

B.P. 14130

DAKAR PEYTAVIN

Senegal

Tel: +221 33 869 0369 / direct: +221 33 869 03 93

Fax: +221 33 869 0370

E-mail: mously.diene@artp.sn; mamadou.faye@artp.sn

URL: www.artp.sn

Communication of 30.VI.2021:

The *Autorité de Régulation des Télécommunications et des Postes (ARTP)*, Dakar, announces the following update of the national numbering plan (NNP) for telephony in Senegal.

*Description of introduction of new resource for national numbering plan for country code 221:*

| *National destination code (NDC) or leading digits of national (significant) number (N(S)N)* | *N(S)N number length* | | *Usage of  ITU-T E.164 number* | *Time and date of introduction* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| 7501 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 23 January 2021 |
| 7533 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 23 January 2021 |
| 7574 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 06 January 2021 |
| 7583 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 23 January 2021 |
| 7563 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 23 January 2021 |
| 7563 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 09 January 2019 |
| 7552 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 09 January 2019 |
| 7544 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 09 January 2019 |
| 7570 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) ORIGINES SA | 28 June 2019 |
| 93310 | 9 | 9 | Non-geographic number – fixed VoIP telephony services for the internet service provider  ARC TELECOM SA | 12 June 2020 |
| 93929 | 9 | 9 | Non-geographic number – fixed VoIP telephony services for the internet service provider  WAW SAS | 04 January 2021 |

*Presentation of national numbering plan for country code 221:*

a) Overview:

The minimum number length (excluding the country code) is **9** digits.

The maximum number length (excluding the country code) is **9** digits.

b) Link to the national database (or any applicable list) with assigned ITU-T E.164 numbers within the national numbering plan (if any): n/a

c) Link to the real-time database reflecting ported ITU-T E.164 numbers (if any):n/a

d) Detail of numbering plan:

| *National destination code (NDC) or leading digits of national (significant) number (N(S)N)* | *N(S)N number length* | | *Usage of  ITU-T E.164 number* | *Additional information* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| 30 | 9 | 9 | Non-geographic number – Fixed telephony service | Operator Expresso Sénégal |
| 32 | 9 | 9 | Non-geographic number – Fixed telephony service | Operator FREE Sénégal |
| 338 | 9 | 9 | Geographic number –  Fixed telephony service | Operator SONATEL (Orange), region of Dakar |
| 339 | 9 | 9 | Geographic number –  Fixed telephony service | Operator SONATEL (Orange), other regions |
| 36 | 9 | 9 | Non-geographic number –  Fixed telephony service | Operator CSU SA (HAYO) |
| 39 | 9 | 9 | Non-geographic number –  Fixed telephony service | ADIE |
| 70 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator Expresso Sénégal |
| 72 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator CSU SA (HAYO) |
| 75 | 9 | 9 | Non-geographic number – Mobile telephone service | Dedicated for mobile virtual network operators (MVNO) |
| 76 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator FREE Sénégal |
| 77 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator SONATEL (Orange) |
| 78 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator SONATEL (Orange) |
| 79 | 9 | 9 | Non-geographic number – Mobile telephone service | ADIE |
| 93 | 9 | 9 | Non-geographic number – Fixed Voice over Internet Protocol (VoIP) telephony service | Dedicated for internet service providers (*Fournisseurs d’accès à internet (FAI)*) |

Contact:

Ms Mana AIDARA and Mr Mamadou Ousmane FAYE

Autorité de Régulation des Télécommunications et des Postes (ARTP)

B.P. 14130

DAKAR PEYTAVIN

Senegal

Tel: +221 33 869 0369 / direct: +221 33 869 03 93

Fax: +221 33 869 0370

E-mail: mana.aidara@artp.sn; mamadou.faye@artp.sn

URL: www.artp.sn

Communication of 1.X.2020:

The *Autorité de Régulation des Télécommunications et des Postes (ARTP)*, Dakar, announces the following update of the national numbering plan (NNP) for telephony in Senegal.

*Description of introduction of new resource for national numbering plan for country code 221:*

| *National destination code (NDC) or leading digits of national (significant) number (N(S)N)* | *N(S)N number length* | | *Usage of  ITU-T E.164 number* | *Time and date of introduction* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| 754 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 09 January 2019 |
| 755 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 09 January 2019 |
| 756 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) SIRIUS TELECOMS AFRIQUE (PROMOBILE) | 09 January 2019 |
| 757 | 9 | 9 | Non-geographic number – Mobile telephone service for the mobile virtual network operator (MVNO) ORIGINES SA | 28 June 2019 |

*Presentation of national numbering plan   
for country code 221:*

a) Overview:

The minimum number length (excluding the country code) is **9**  digits.  
 The maximum number length (excluding the country code) is **9**  digits.

b) Link to the national database (or any applicable list) with assigned ITU-T E.164 numbers within the national numbering plan (if any): n/a

c) Link to the real-time database reflecting ported ITU-T E.164 numbers (if any):n/a

d) Detail of numbering plan:

| *National destination code (NDC) or leading digits of national (significant) number (N(S)N)* | *N(S)N number length* | | *Usage of  ITU-T E.164 number* | *Additional information* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| 30 | 9 | 9 | Non-geographic number – Fixed telephony service | Operator Expresso Sénégal |
| 32 | 9 | 9 | Non-geographic number – Fixed telephony service | Operator FREE Sénégal |
| 338 | 9 | 9 | Geographic number –  Fixed telephony service | Operator SONATEL (Orange), Région de Dakar |
| 339 | 9 | 9 | Geographic number –  Fixed telephony service | Operator SONATEL (Orange), autres régions |
| 3611 | 9 | 9 | Non-geographic number – Fixed telephony service | Operator CSU SA (HAYO) |
| 390 | 9 | 9 | Non-geographic number – Fixed telephony service | ADIE |
| 391 | 9 | 9 | Non-geographic number – Fixed telephony service | ADIE |
| 70 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator Expresso Sénégal |
| 7211 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator CSU SA (HAYO) |
| 754 | 9 | 9 | Non-geographic number – Mobile telephone service | MVNO PROMOBILE |
| 755 | 9 | 9 | Non-geographic number – Mobile telephone service | MVNO PROMOBILE |
| 756 | 9 | 9 | Non-geographic number – Mobile telephone service | MVNO PROMOBILE |
| 757 | 9 | 9 | Non-geographic number – Mobile telephone service | MVNO ORIGINES SA |
| 76 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator FREE Sénégal |
| 77 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator SONATEL (Orange) |
| 78 | 9 | 9 | Non-geographic number – Mobile telephone service | Operator SONATEL (Orange) |
| 790 | 9 | 9 | Non-geographic number – Mobile telephone service | ADIE |

Contact:

Ms Mana AIDARA and Mr Mamadou Ousmane FAYE   
Autorité de Régulation des Télécommunications et des Postes (ARTP)  
B.P. 14130  
DAKAR PEYTAVIN  
Senegal  
Tel: +221 33 869 0369 / direct: +221 33 869 03 93  
Fax: +221 33 869 0370  
E-mail: mana.aidara@artp.sn; [mamadou.faye@artp.sn](mailto:mamadou.faye@artp.sn)  
URL: www.artp.sn

Communication of 1.IV.2016:

The *Autorité de Régulation des Télécommunications et des Postes (ARTP)*, Dakar, announces the following update of the National Numbering Plan (NNP) for telephony in Senegal. The NNP is a closed, nine-digit plan with the following format:

CC N(S)N

where:

CC (Country Code) = +221

N(S)N (National (Significant) Number) comprising nine digits: SABPQMCDU

**I) Incoming international calls**

International numbering format: CC (221) + N(S)N (nine digits)

1. **Mobile telephony numbers**

The blocks of numbers for which "**S**" is "**7**" are reserved for the mobile telephony networks.

– The list of numbers SABPQMCDU currently allocated to the universal service operator CSU-SA for its mobile phone network is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of E.164 number** | **Additional information** |
| **Prefix** | **BP/BPQ** | **Maximum length** | **Minimum length** |
|
|
|
| 72 | 110 XXXX | 9 | 9 | CDMA Mobile | CSU |
| 72 | 111 XXXX | 9 | 9 | CDMA Mobile |
| 72 | 112 XXXX | 9 | 9 | CDMA Mobile |

– The list of numbers SABPQMCDU currently allocated to the operator Expresso Sénégal for its mobile phone network is as follows:

| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| --- | --- | --- | --- | --- | --- |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 70 | 00X XXXX | 9 | 9 | Baneex/Prepaid | Expresso Sénégal |
| 70 | 10X XXXX | 9 | 9 | Baneex |
| 70 | 20X XXXX | 9 | 9 | Baneex |
| 70 | 30X XXXX | 9 | 9 | GSM |
| 70 | 32X XXXX | 9 | 9 | GSM |
| 70 | 33X XXXX | 9 | 9 | GSM |
| 70 | 34X XXXX | 9 | 9 | GSM |
| 70 | 35X XXXX | 9 | 9 | GSM |
| 70 | 36X XXXX | 9 | 9 | GSM |
| 70 | 40X XXXX | 9 | 9 | GSM |
| 70 | 45X XXXX | 9 | 9 | GSM |
| 70 | 46X XXXX | 9 | 9 | GSM |
| 70 | 47X XXXX | 9 | 9 | GSM |
| 70 | 48X XXXX | 9 | 9 | GSM |
| 70 | 49X XXXX | 9 | 9 | GSM |
| 70 | 50X XXXX | 9 | 9 | Baneex |
| 70 | 51X XXXX | 9 | 9 | GSM |
| 70 | 52X XXXX | 9 | 9 | GSM |
| 70 | 56X XXXX | 9 | 9 | GSM |
| 70 | 57X XXXX | 9 | 9 | GSM |
| 70 | 58X XXXX | 9 | 9 | GSM |
| 70 | 59X XXXX | 9 | 9 | GSM |
| 70 | 60X XXXX | 9 | 9 | GSM |
| 70 | 61X XXXX | 9 | 9 | GSM |
| 70 | 62X XXXX | 9 | 9 | GSM |
| 70 | 63X XXXX | 9 | 9 | GSM |
| 70 | 64X XXXX | 9 | 9 | GSM/Prepaid |
| 70 | 65X XXXX | 9 | 9 | GSM |
| 70 | 67X XXXX | 9 | 9 | GSM |
| 70 | 68X XXXX | 9 | 9 | GSM | Expresso Sénégal |
| 70 | 69X XXXX | 9 | 9 | GSM |
| 70 | 70X XXXX | 9 | 9 | Baneex |
| 70 | 71X XXXX | 9 | 9 | GSM |
| 70 | 72X XXXX | 9 | 9 | GSM |
| 70 | 73X XXXX | 9 | 9 | GSM |
| 70 | 74X XXXX | 9 | 9 | GSM |
| 70 | 75X XXXX | 9 | 9 | GSM |
| 70 | 76X XXXX | 9 | 9 | GSM |
| 70 | 77X XXXX | 9 | 9 | GSM/Prepaid |
| 70 | 78X XXXX | 9 | 9 | GSM |
| 70 | 79X XXXX | 9 | 9 | GSM |
| 70 | 80X XXXX | 9 | 9 | GSM |
| 70 | 81X XXXX | 9 | 9 | GSM |
| 70 | 82X XXXX | 9 | 9 | GSM |
| 70 | 83X XXXX | 9 | 9 | GSM |
| 70 | 84X XXXX | 9 | 9 | GSM |
| 70 | 87X XXXX | 9 | 9 | GSM |
| 70 | 88X XXXX | 9 | 9 | GSM |
| 70 | 89X XXXX | 9 | 9 | GSM |
| 70 | 90X XXXX | 9 | 9 | GSM |
| 70 | 91X XXXX | 9 | 9 | GSM |
| 70 | 92X XXXX | 9 | 9 | GSM |
| 70 | 93X XXXX | 9 | 9 | GSM |
| 70 | 94X XXXX | 9 | 9 | GSM |
| 70 | 95X XXXX | 9 | 9 | GSM |
| 70 | 96X XXXX | 9 | 9 | GSM |
| 70 | 97X XXXX | 9 | 9 | GSM |
| 70 | 98X XXXX | 9 | 9 | GSM |

– The list of numbers SABPQMCDU currently allocated to the operator Sentel GSM « Tigo » for its mobile phone network is as follows:

| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| --- | --- | --- | --- | --- | --- |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 76 | 01X XXXX | 9 | 9 | Mobile GSM | Sentel GSM (Tigo) |
| 76 | 02X XXXX | 9 | 9 | Mobile GSM |
| 76 | 12X XXXX | 9 | 9 | Mobile GSM |
| 76 | 13X XXXX | 9 | 9 | Mobile GSM |
| 76 | 28X XXXX | 9 | 9 | Mobile GSM |
| 76 | 29X XXXX | 9 | 9 | Mobile GSM |
| 76 | 30X XXXX | 9 | 9 | Mobile GSM |
| 76 | 31X XXXX | 9 | 9 | Mobile GSM |
| 76 | 32X XXXX | 9 | 9 | Mobile GSM |
| 76 | 33X XXXX | 9 | 9 | Mobile GSM |
| 76 | 34X XXXX | 9 | 9 | Mobile GSM |
| 76 | 35X XXXX | 9 | 9 | Mobile GSM |
| 76 | 36X XXXX | 9 | 9 | Mobile GSM |
| 76 | 37X XXXX | 9 | 9 | Mobile GSM |
| 76 | 38X XXXX | 9 | 9 | Mobile GSM |
| 76 | 39X XXXX | 9 | 9 | Mobile GSM |
| 76 | 45X XXXX | 9 | 9 | Mobile GSM |
| 76 | 46X XXXX | 9 | 9 | Mobile GSM |
| 76 | 47X XXXX | 9 | 9 | Mobile GSM |
| 76 | 48X XXXX | 9 | 9 | Mobile GSM |
| 76 | 49X XXXX | 9 | 9 | Mobile GSM |
| 76 | 50X XXXX | 9 | 9 | Mobile GSM |
| 76 | 51X XXXX | 9 | 9 | Mobile GSM |
| 76 | 52X XXXX | 9 | 9 | Mobile GSM |
| 76 | 53X XXXX | 9 | 9 | Mobile GSM |
| 76 | 54X XXXX | 9 | 9 | Mobile GSM |
| 76 | 55X XXXX | 9 | 9 | Mobile GSM |
| 76 | 56X XXXX | 9 | 9 | Mobile GSM |
| 76 | 57X XXXX | 9 | 9 | Mobile GSM |
| 76 | 58X XXXX | 9 | 9 | Mobile GSM |
| 76 | 59X XXXX | 9 | 9 | Mobile GSM |

| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| --- | --- | --- | --- | --- | --- |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 76 | 60X XXXX | 9 | 9 | Mobile GSM | Sentel GSM (Tigo) |
| 76 | 61X XXXX | 9 | 9 | Mobile GSM |
| 76 | 63X XXXX | 9 | 9 | Mobile GSM |
| 76 | 64X XXXX | 9 | 9 | Mobile GSM |
| 76 | 65X XXXX | 9 | 9 | Mobile GSM |
| 76 | 66X XXXX | 9 | 9 | Mobile GSM |
| 76 | 67X XXXX | 9 | 9 | Mobile GSM |
| 76 | 68X XXXX | 9 | 9 | Mobile GSM |
| 76 | 69X XXXX | 9 | 9 | Mobile GSM |
| 76 | 72X XXXX | 9 | 9 | Mobile GSM |
| 76 | 73X XXXX | 9 | 9 | Mobile GSM |
| 76 | 74X XXXX | 9 | 9 | Mobile GSM |
| 76 | 75X XXXX | 9 | 9 | Mobile GSM |
| 76 | 83X XXXX | 9 | 9 | Mobile GSM |
| 76 | 84X XXXX | 9 | 9 | Mobile GSM |
| 76 | 85X XXXX | 9 | 9 | Mobile GSM |
| 76 | 86X XXXX | 9 | 9 | Mobile GSM |
| 76 | 87X XXXX | 9 | 9 | Mobile GSM |
| 76 | 88X XXXX | 9 | 9 | Mobile GSM |
| 76 | 90X XXXX | 9 | 9 | Mobile GSM |
| 76 | 92X XXXX | 9 | 9 | Mobile GSM |
| 76 | 94X XXXX | 9 | 9 | Mobile GSM |

– The list of numbers SABPQMCDU currently allocated to the operator Sonatel on behalf of its mobile subsidiary Sonatel Mobiles « Orange » is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
| 77 | 01X XXXX | 9 | 9 | Mobile GSM | Sonatel Mobiles (Orange) |
| 77 | 02X XXXX | 9 | 9 | Mobile GSM |
| 77 | 03X XXXX | 9 | 9 | Mobile GSM |
| 77 | 04X XXXX | 9 | 9 | Mobile GSM |
| 77 | 05X XXXX | 9 | 9 | Mobile GSM |
| 77 | 06X XXXX | 9 | 9 | Mobile GSM |
| 77 | 07X XXXX | 9 | 9 | Mobile GSM |
| 77 | 08X XXXX | 9 | 9 | Mobile GSM |
| 77 | 09X XXXX | 9 | 9 | Mobile GSM |
| 77 | 10X XXXX | 9 | 9 | Mobile GSM |
| 77 | 11X XXXX | 9 | 9 | Mobile GSM |
| 77 | 12X XXXX | 9 | 9 | Mobile GSM |
| 77 | 13X XXXX | 9 | 9 | Mobile GSM |
| 77 | 14X XXXX | 9 | 9 | Mobile GSM |
| 77 | 15X XXXX | 9 | 9 | Mobile GSM |
| 77 | 16X XXXX | 9 | 9 | Mobile GSM |
| 77 | 17X XXXX | 9 | 9 | Mobile GSM |
| 77 | 18X XXXX | 9 | 9 | Mobile GSM |
| 77 | 19X XXXX | 9 | 9 | Mobile GSM |
| 77 | 20X XXXX | 9 | 9 | Mobile GSM |
| 77 | 21X XXXX | 9 | 9 | Mobile GSM |
| 77 | 22X XXXX | 9 | 9 | Mobile GSM |
| 77 | 23X XXXX | 9 | 9 | Mobile GSM |
| 77 | 24X XXXX | 9 | 9 | Mobile GSM |
| 77 | 25X XXXX | 9 | 9 | Mobile GSM |
| 77 | 26X XXXX | 9 | 9 | Mobile GSM |
| 77 | 27X XXXX | 9 | 9 | Mobile GSM |
| 77 | 28X XXXX | 9 | 9 | Mobile GSM |
| 77 | 29X XXXX | 9 | 9 | Mobile GSM |
| 77 | 30X XXXX | 9 | 9 | Mobile GSM |
| 77 | 31X XXXX | 9 | 9 | Mobile GSM |
| 77 | 32X XXXX | 9 | 9 | Mobile GSM |
| 77 | 33X XXXX | 9 | 9 | Mobile GSM |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 77 | 34X XXXX | 9 | 9 | Mobile GSM | Sonatel Mobiles (Orange) |
| 77 | 35X XXXX | 9 | 9 | Mobile GSM |
| 77 | 36X XXXX | 9 | 9 | Mobile GSM |
| 77 | 37X XXXX | 9 | 9 | Mobile GSM |
| 77 | 38X XXXX | 9 | 9 | Mobile GSM |
| 77 | 39X XXXX | 9 | 9 | Mobile GSM |
| 77 | 40X XXXX | 9 | 9 | Mobile GSM |
| 77 | 41X XXXX | 9 | 9 | Mobile GSM |
| 77 | 42X XXXX | 9 | 9 | Mobile GSM |
| 77 | 43X XXXX | 9 | 9 | Mobile GSM |
| 77 | 44X XXXX | 9 | 9 | Mobile GSM |
| 77 | 45X XXXX | 9 | 9 | Mobile GSM |
| 77 | 46X XXXX | 9 | 9 | Mobile GSM |
| 77 | 47X XXXX | 9 | 9 | Mobile GSM |
| 77 | 48X XXXX | 9 | 9 | Mobile GSM |
| 77 | 49X XXXX | 9 | 9 | Mobile GSM |
| 77 | 50X XXXX | 9 | 9 | Mobile GSM |
| 77 | 51X XXXX | 9 | 9 | Mobile GSM |
| 77 | 52X XXXX | 9 | 9 | Mobile GSM |
| 77 | 53X XXXX | 9 | 9 | Mobile GSM |
| 77 | 54X XXXX | 9 | 9 | Mobile GSM |
| 77 | 55X XXXX | 9 | 9 | Mobile GSM |
| 77 | 56X XXXX | 9 | 9 | Mobile GSM |
| 77 | 57X XXXX | 9 | 9 | Mobile GSM |
| 77 | 58X XXXX | 9 | 9 | Mobile GSM |
| 77 | 59X XXXX | 9 | 9 | Mobile GSM |
| 77 | 60X XXXX | 9 | 9 | Mobile GSM |
| 77 | 61X XXXX | 9 | 9 | Mobile GSM |
| 77 | 62X XXXX | 9 | 9 | Mobile GSM |
| 77 | 63X XXXX | 9 | 9 | Mobile GSM |
| 77 | 64X XXXX | 9 | 9 | Mobile GSM |
| 77 | 65X XXXX | 9 | 9 | Mobile GSM |
| 77 | 66X XXXX | 9 | 9 | Mobile GSM |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 77 | 67X XXXX | 9 | 9 | Mobile GSM | Sonatel Mobiles (Orange) |
| 77 | 68X XXXX | 9 | 9 | Mobile GSM |
| 77 | 69X XXXX | 9 | 9 | Mobile GSM |
| 77 | 70X XXXX | 9 | 9 | Mobile GSM |
| 77 | 71X XXXX | 9 | 9 | Mobile GSM |
| 77 | 72X XXXX | 9 | 9 | Mobile GSM |
| 77 | 73X XXXX | 9 | 9 | Mobile GSM |
| 77 | 74X XXXX | 9 | 9 | Mobile GSM |
| 77 | 75X XXXX | 9 | 9 | Mobile GSM |
| 77 | 76X XXXX | 9 | 9 | Mobile GSM |
| 77 | 77X XXXX | 9 | 9 | Mobile GSM |
| 77 | 78X XXXX | 9 | 9 | Mobile GSM |
| 77 | 79X XXXX | 9 | 9 | Mobile GSM |
| 77 | 80X XXXX | 9 | 9 | Mobile GSM |
| 77 | 81X XXXX | 9 | 9 | Mobile GSM |
| 77 | 82X XXXX | 9 | 9 | Mobile GSM |
| 77 | 83X XXXX | 9 | 9 | Mobile GSM |
| 77 | 84X XXXX | 9 | 9 | Mobile GSM |
| 77 | 85X XXXX | 9 | 9 | Mobile GSM |
| 77 | 86X XXXX | 9 | 9 | Mobile GSM |
| 77 | 87X XXXX | 9 | 9 | Mobile GSM |
| 77 | 88X XXXX | 9 | 9 | Mobile GSM |
| 77 | 89X XXXX | 9 | 9 | Mobile GSM |
| 77 | 90X XXXX | 9 | 9 | Mobile GSM |
| 77 | 91X XXXX | 9 | 9 | Mobile GSM |
| 77 | 92X XXXX | 9 | 9 | Mobile GSM |
| 77 | 93X XXXX | 9 | 9 | Mobile GSM |
| 77 | 94X XXXX | 9 | 9 | Mobile GSM |
| 77 | 95X XXXX | 9 | 9 | Mobile GSM |
| 77 | 96X XXXX | 9 | 9 | Mobile GSM |
| 77 | 97X XXXX | 9 | 9 | Mobile GSM |
| 77 | 98X XXXX | 9 | 9 | Mobile GSM |
| 77 | 99X XXXX | 9 | 9 | Mobile GSM |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 78 | 01X XXXX | 9 | 9 | Mobile GSM | Sonatel Mobiles (Orange) |
| 78 | 10X XXXX | 9 | 9 | Mobile GSM |
| 78 | 11X XXXX | 9 | 9 | Mobile GSM |
| 78 | 12X XXXX | 9 | 9 | Mobile GSM |
| 78 | 13X XXXX | 9 | 9 | Mobile GSM |
| 78 | 14X XXXX | 9 | 9 | Mobile GSM |
| 78 | 15X XXXX | 9 | 9 | Mobile GSM |
| 78 | 16X XXXX | 9 | 9 | Mobile GSM |
| 78 | 17X XXXX | 9 | 9 | Mobile GSM |
| 78 | 18X XXXX | 9 | 9 | Mobile GSM |
| 78 | 19X XXXX | 9 | 9 | Mobile GSM |
| 78 | 20X XXXX | 9 | 9 | Mobile GSM |
| 78 | 21X XXXX | 9 | 9 | Mobile GSM |
| 78 | 22X XXXX | 9 | 9 | Mobile GSM |
| 78 | 23X XXXX | 9 | 9 | Mobile GSM |
| 78 | 24X XXXX | 9 | 9 | Mobile GSM |
| 78 | 25X XXXX | 9 | 9 | Mobile GSM |
| 78 | 26X XXXX | 9 | 9 | Mobile GSM |
| 78 | 27X XXXX | 9 | 9 | Mobile GSM |
| 78 | 28X XXXX | 9 | 9 | Mobile GSM |
| 78 | 29X XXXX | 9 | 9 | Mobile GSM |
| 78 | 30X XXXX | 9 | 9 | Mobile GSM |
| 78 | 31X XXXX | 9 | 9 | Mobile GSM |
| 78 | 32X XXXX | 9 | 9 | Mobile GSM |
| 78 | 33X XXXX | 9 | 9 | Mobile GSM |
| 78 | 34X XXXX | 9 | 9 | Mobile GSM |
| 78 | 35X XXXX | 9 | 9 | Mobile GSM |
| 78 | 36X XXXX | 9 | 9 | Mobile GSM |
| 78 | 37X XXXX | 9 | 9 | Mobile GSM |
| 78 | 38X XXXX | 9 | 9 | Mobile GSM |
| 78 | 39X XXXX | 9 | 9 | Mobile GSM |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 78 | 40X XXXX | 9 | 9 | Mobile GSM | Sonatel Mobiles (Orange) |
| 78 | 41X XXXX | 9 | 9 | Mobile GSM |
| 78 | 42X XXXX | 9 | 9 | Mobile GSM |
| 78 | 43X XXXX | 9 | 9 | Mobile GSM |
| 78 | 44X XXXX | 9 | 9 | Mobile GSM |
| 78 | 45X XXXX | 9 | 9 | Mobile GSM |
| 78 | 46X XXXX | 9 | 9 | Mobile GSM |
| 78 | 47X XXXX | 9 | 9 | Mobile GSM |
| 78 | 48X XXXX | 9 | 9 | Mobile GSM |
| 78 | 49X XXXX | 9 | 9 | Mobile GSM |
| 78 | 63X XXXX | 9 | 9 | Mobile GSM |

– The list of numbers SABPQMCDU currently allocated to the State (ADIE) for the operation of its mobile phone network is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of  E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
| 79 | 00X XXXX | 9 | 9 | CDMA Mobile | ADIE |
| 79 | 01X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 02X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 03X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 04X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 05X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 06X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 07X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 08X XXXX | 9 | 9 | CDMA Mobile |
| 79 | 09X XXXX | 9 | 9 | CDMA Mobile |

1. **Fixed telephony numbers**

The blocks of numbers for which "**S**" is "**3**" are reserved for the fixed telephony networks.

– The list of numbers SABPQMCDU currently allocated to the operator Expresso Sénégal for its fixed telephony network is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 30 | 10X XXXX | 9 | 9 | CDMA fixed telephony | Expresso Sénégal |
| 30 | 11X XXXX | 9 | 9 | CDMA fixed telephony |
| 30 | 12X XXXX | 9 | 9 | CDMA fixed telephony |
| 30 | 80X XXXX | 9 | 9 | CDMA fixed telephony |

– The list of numbers SABPQMCDU currently allocated to the universal service operator CSU-SA for its fixed telephony network is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of E.164 number** | **Additional information** |
| **Prefix** | **BP/BPQ** | **Maximum length** | **Minimum length** |
|
|
|
| 36 | 111 XXXX | 9 | 9 | CDMA fixed wireless | CSU |

– The list of numbers SABPQMCDU currently allocated to the operator Sentel GSM (Tigo) for the operation of its fixed telephony network is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 32 | 824 XXXX | 9 | 9 | GSM fixed telephony service | Sentel GSM (Tigo) |

– The list of numbers SABPQMCDU currently allocated to the State (ADIE) for the operation of its fixed telephony network is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 39 | 00X XXXX | 9 | 9 | VoIP, PABX, IPBX | ADIE |
| 39 | 01X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 02X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 03X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 04X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 05X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 06X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 07X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 08X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 09X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 10X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 11X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 12X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 13X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 14X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 15X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 16X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 17X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 18X XXXX | 9 | 9 | VoIP, PABX, IPBX |
| 39 | 19X XXXX | 9 | 9 | VoIP, PABX, IPBX |

– The list of numbers SABPQMCDU currently allocated to the operator Sonatel for its fixed telephony network is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **N(S)N\* (NDC + SN)** | | **N(S)N length** | | **Usage of E.164 number** | **Additional information** |
| **Prefix** | **BP** | **Maximum length** | **Minimum length** |
|
|
|
| 33 | 81X XXXX | 9 | 9 | Fixed telephony service | Sonatel (Orange) |
| 33 | 82X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 83X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 84X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 85X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 86X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 87X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 88X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 89X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 92X XXXX | 9 | 9 | Satellite telephony |
| 33 | 93X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 94X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 95X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 96X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 97X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 98X XXXX | 9 | 9 | Fixed telephony service |
| 33 | 99X XXXX | 9 | 9 | Fixed telephony service |

**II) National calls**

In order to call a subscriber to the public national fixed or mobile telecommunication networks (local or national call), a number in the format SABPQMCDU is used.

**III) Calls to emergency services**

The numbers used to contact one of the emergency services (two or three digits) from within the country take the following format:

1X - where X = 8 fire service and X = 7 police

These services cannot be called from outside the country.

**IV) Outgoing international calls**

In order to make an international call from Senegal, dial the international prefix “00” and then the number in the following format:

00 CC NDC SN, where:

| CC | = | Country Code |
| --- | --- | --- |
| NDC | = | National Destination Code |
| SN | = | Subscriber Number |

**V) Non-geographical numbers (convergent services: IP telephony, etc.)**

These numbers take the form SABPQMCDU, in which S = 9.

– The list of numbers SABPQMCDU currently allocated to the operator Sonatel for its converged services network is 93 330 XXXX.

Contact:

Ms Mana AIDARA and Mr Mamadou Ousmane FAYE

Autorité de Régulation des Télécommunications et des Postes (ARTP)

B.P. 14130

DAKAR PEYTAVIN

Senegal

Tel: +221 33 869 0369 / direct: +221 33 869 03 93

Fax: +221 33 869 0370

E-mail: mana.aidara@artp.sn; mamadou.faye@artp.sn

URL: www.artp.sn