**Togo (country code +228)**

Communication of 11.I.2021:

The *Autorité de Régulation des Communications Électroniques et des Postes (ARCEP)*, Lomé, announces the national numbering plan of Togo.

(a) Overview:

Maximum number length (not including country code): 8 digits

Minimum number length (not including country code): 8 digits

(b) Details of numbering plan

| *NDC (national destination code)  or leading digits of N(S)N (national (significant) number)* | *N(S)N number length* | | *Usage of  E.164 number* | *Additional information* |
| --- | --- | --- | --- | --- |
| *Maximum length* | *Minimum length* |
| * *Geographical numbers* | | | | |
| 220 | 8 digits | 8 digits | Fixed telephony, Lomé | Not allocated |
| 221 | 8 digits | 8 digits | Not allocated |
| 222 | 8 digits | 8 digits | TOGO TELECOM |
| 223 | 8 digits | 8 digits | Not allocated |
| 224 | 8 digits | 8 digits | Not allocated |
| 225 | 8 digits | 8 digits | TOGO TELECOM |
| 226 | 8 digits | 8 digits | TOGO TELECOM |
| 227 | 8 digits | 8 digits | Not allocated |
| 228 | 8 digits | 8 digits | Not allocated |
| 229 | 8 digits | 8 digits | Not allocated |
| 230 | 8 digits | 8 digits | Fixed telephony, Maritime region | Not allocated |
| 231 | 8 digits | 8 digits | Not allocated |
| 232 | 8 digits | 8 digits | Not allocated |
| 233 | 8 digits | 8 digits | TOGO TELECOM |
| 234 | 8 digits | 8 digits | Not allocated |
| 235 | 8 digits | 8 digits | Not allocated |
| 236 | 8 digits | 8 digits | Not allocated |
| 237 | 8 digits | 8 digits | Not allocated |
| 238 | 8 digits | 8 digits | Not allocated |
| 239 | 8 digits | 8 digits | Not allocated |
| 240 | 8 digits | 8 digits | Fixed telephony, Plateaux region | Not allocated |
| 241 | 8 digits | 8 digits | Not allocated |
| 242 | 8 digits | 8 digits | Not allocated |
| 243 | 8 digits | 8 digits | Not allocated |
| 244 | 8 digits | 8 digits | TOGO TELECOM |
| 245 | 8 digits | 8 digits | Not allocated |
| 246 | 8 digits | 8 digits | Not allocated |
| 247 | 8 digits | 8 digits | Not allocated |
| 248 | 8 digits | 8 digits | Not allocated |
| 249 | 8 digits | 8 digits | Not allocated |
| 250 | 8 digits | 8 digits | Fixed telephony, Central region | Not allocated |
| 251 | 8 digits | 8 digits | Not allocated |
| 252 | 8 digits | 8 digits | Not allocated |
| 253 | 8 digits | 8 digits | Not allocated |
| 254 | 8 digits | 8 digits | Not allocated |
| 255 | 8 digits | 8 digits | TOGO TELECOM |
| 256 | 8 digits | 8 digits | Not allocated |
| 257 | 8 digits | 8 digits | Not allocated |
| 258 | 8 digits | 8 digits | Not allocated |
| 259 | 8 digits | 8 digits | Not allocated |
| 260 | 8 digits | 8 digits | Fixed telephony, Kara region | Not allocated |
| 261 | 8 digits | 8 digits | Not allocated |
| 262 | 8 digits | 8 digits | Not allocated |
| 263 | 8 digits | 8 digits | Not allocated |
| 264 | 8 digits | 8 digits | Not allocated |
| 265 | 8 digits | 8 digits | Not allocated |
| 266 | 8 digits | 8 digits | TOGO TELECOM |
| 267 | 8 digits | 8 digits | Not allocated |
| 268 | 8 digits | 8 digits | Not allocated |
| 269 | 8 digits | 8 digits | Not allocated |
| 270 | 8 digits | 8 digits | Fixed telephony, savannah region | Not allocated |
| 271 | 8 digits | 8 digits | Not allocated |
| 272 | 8 digits | 8 digits | Not allocated |
| 273 | 8 digits | 8 digits | Not allocated |
| 274 | 8 digits | 8 digits | Not allocated |
| 275 | 8 digits | 8 digits | Not allocated |
| 276 | 8 digits | 8 digits | Not allocated |
| 277 | 8 digits | 8 digits | TOGO TELECOM |
| 278 | 8 digits | 8 digits | Not allocated |
| 279 | 8 digits | 8 digits | Not allocated |
| * *Non-geographical numbers* | | | | |
| 90 | 8 digits | 8 digits | Mobile telephony | TOGO CELLULAIRE |
| 91 | 8 digits | 8 digits |
| 92 | 8 digits | 8 digits |
| 93 | 8 digits | 8 digits |
| 94 | 8 digits | 8 digits | Not allocated |
| 95 | 8 digits | 8 digits | Not allocated |
| 96 | 8 digits | 8 digits | ATLANTIQUE TELECOM TOGO |
| 97 | 8 digits | 8 digits |
| 98 | 8 digits | 8 digits |
| 99 | 8 digits | 8 digits |
| 700 to 705 | 8 digits | 8 digits | Mobile telephony | TOGO CELLULAIRE |
| 706 to 709 | 8 digits | 8 digits | Not allocated |
| 71 | 8 digits | 8 digits | Not allocated |
| 72 | 8 digits | 8 digits | Not allocated |
| 73 | 8 digits | 8 digits | Not allocated |
| 74 | 8 digits | 8 digits | Not allocated |
| 75 | 8 digits | 8 digits | Not allocated |
| 76 | 8 digits | 8 digits | Not allocated |
| 77 | 8 digits | 8 digits | Not allocated |
| 78 | 8 digits | 8 digits | Not allocated |
| 790 to 792 | 8 digits | 8 digits | Not allocated |
| 793 to 799 | 8 digits | 8 digits | ATLANTIQUE TELECOM TOGO |

Contact:

Ms Adzowavi Massan GNOGNO

Autorité de Régulation des Communications Électroniques et des Postes (ARCEP)

4638, Boulevard Général Gnassingbé Eyadema – Immeuble ARCEP

BP 358 LOMÉ

Togo

Tel: +228 22 23 63 80

Fax: +228 22 23 63 94 / 22 61 70 82

E-mail: arcep@arcep.tg ; jeanne.gnogno@arcep.tg

URL: www.arcep.tg