|  |
| --- |
| **Recommendation ITU-R P.313-11**  **(02/2012)** |
| **Exchange of information for short-term forecasts and transmission of ionospheric disturbance warnings** |
| **P Series**  **Radiowave propagation** |

Foreword

The role of the Radiocommunication Sector is to ensure the rational, equitable, efficient and economical use of the radio-frequency spectrum by all radiocommunication services, including satellite services, and carry out studies without limit of frequency range on the basis of which Recommendations are adopted.

The regulatory and policy functions of the Radiocommunication Sector are performed by World and Regional Radiocommunication Conferences and Radiocommunication Assemblies supported by Study Groups.

# Policy on Intellectual Property Right (IPR)

ITU-R policy on IPR is described in the Common Patent Policy for ITU-T/ITU-R/ISO/IEC referenced in Annex 1 of Resolution ITU-R 1. Forms to be used for the submission of patent statements and licensing declarations by patent holders are available from <http://www.itu.int/ITU-R/go/patents/en> where the Guidelines for Implementation of the Common Patent Policy for ITU‑T/ITU‑R/ISO/IEC and the ITU-R patent information database can also be found.

|  |  |
| --- | --- |
| Series of ITU-R Recommendations  (Also available online at <http://www.itu.int/publ/R-REC/en>) | |
| **Series** | Title |
| **BO** | Satellite delivery |
| **BR** | Recording for production, archival and play-out; film for television |
| **BS** | Broadcasting service (sound) |
| **BT** | Broadcasting service (television) |
| **F** | Fixed service |
| **M** | Mobile, radiodetermination, amateur and related satellite services |
| P | Radiowave propagation |
| **RA** | Radio astronomy |
| **RS** | Remote sensing systems |
| **S** | Fixed-satellite service |
| **SA** | Space applications and meteorology |
| **SF** | Frequency sharing and coordination between fixed-satellite and fixed service systems |
| **SM** | Spectrum management |
| **SNG** | Satellite news gathering |
| **TF** | Time signals and frequency standards emissions |
| **V** | Vocabulary and related subjects |

|  |
| --- |
|  |

|  |
| --- |
| ***Note***: *This ITU-R Recommendation was approved in English under the procedure detailed in Resolution ITU-R 1.* |

*Electronic Publication*

Geneva, 2012

© ITU 2012

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without written permission of ITU.

RECOMMENDATION ITU-R P.313-11

Exchange of information for short-term forecasts and transmission  
of ionospheric disturbance warnings

(Question ITU-R 213/3)

(1951-1959-1966-1974-1978-1982-1986-1990-1992-1995-1999-2005-2012)

Scope

This Recommendation provides guidance on the submission of meteorological information that could be used to perform short-term forecasts and the transmission of space weather disturbance warnings to ionospheric and trans-ionospheric propagation. It also provides information on the availability and exchange of basic data for radio propagation forecasts and space weather prediction.

The ITU Radiocommunication Assembly,

considering

a) that some radiocommunication services would benefit from having the earliest possible warnings of the probable onset of space weather disturbances to ionospheric and trans-ionospheric propagation;

b) that Annex 1 contains the most recent information on the availability and exchange of basic data for radio propagation forecasts and space weather predictions at a level of solar activity,

recommends

**1** that each country participating in radio propagation research should designate an official agency for the reception, coordination and exchange of information required for the preparation of short-term forecasts, and for liaison with corresponding agencies in other countries;

**2** that such information should be forwarded to the above agencies by the most direct means of telecommunication (e.g. E-mail, web-portal);

**3** that data needed for short-term forecasting in near real-time should be disseminated in accordance with the International Space Environment Service (ISES) and World Meteorological Organization (WMO), Inter-programme Coordination Team on Space Weather (ICTSW) decisions by suitable available communication channels, while other data should be disseminated or made available by electronic means, or, if requested, by other rapid means of communication, and that short regular transmissions giving short-term warnings of ionospheric disturbances should be effected by long‑range radio stations;

**4** that codes to be used for the above communication and dissemination should be fully standardized in accordance with ISES decisions and actions;

**5** that administrations and operating agencies using the above services should be invited to compare the forecasts with the actual behaviour of radio circuits, to evaluate the accuracy of the forecasts throughout the solar cycle, and to provide records and make any suggestions which might assist the studies undertaken to improve the methods used;

**6** that it is desirable that a common method, based on the work on Question ITU-R 213/3 be adopted to describe ionospheric perturbations and variations, for correlation with space weather forecasts and the behaviour of operating radio services;

**7** that, where administrations have provided facilities for the rapid interchange of information in connection with the ISES and the WMO Information System, these facilities should be maintained, and, if necessary, extended in the future.

Annex 1  
  
Availability and exchange of basic data and operational data  
for radio propagation space weather forecasts

# 1 Introduction

Propagation of radio signals in the range 3 to 30 MHz is practicable over any but the shortest distances, mainly because of the possibility of obtaining ionospheric and ground reflections which result in small values of attenuation. Satisfactory communications for a given circuit can generally be obtained if the operating frequency lies between a lower (LUF) and an upper (operational MUF) frequency limit. These are determined by ionospheric characteristics. The operational range of frequencies has been found to be even more restricted with some forms of high capacity communication systems. Recommendation ITU-R P.531 provides for radio propagation prediction method required for the design of satellite services and systems.

Since only a limited range of frequencies can be used, it is desirable to have, as far in advance as possible, information on the probable values of these upper and lower limits, as well as short-term forecasts and disturbance warnings. Collectively, these predictions (long-term) and forecasts (short‑term) and disturbance warnings provide information for planning and operating personnel, that can be utilized in making the most economical use of the limited resources of equipment and frequency spectrum. The long- and medium-term predictions are indicative of representative ionospheric conditions, so that it is extremely useful to operating personnel to be warned of impending ionospheric disturbances in order that traffic can be re-routed, instructions can be issued in advance to cover temporary adjustments in the normal operating frequency, and the performance of other systems affected by the ionosphere can be assessed. Recommendation ITU-R P.533 provides an HF propagation prediction method.

# 2 Available data for radio-propagation forecasts

## 2.1 Long-term predictions

Organizations in several countries prepare predictions of ionospheric conditions and ionospheric indices from 1 month up to 12 months in advance; for general planning purposes, predictions for a complete solar cycle are also made by some organizations. These predictions are for representative ionospheric conditions. The information which is applicable to any part of the world, is available for interchange between the organizations undertaking this service.

## 2.2 Forecasts of disturbances

Organizations in several countries prepare forecasts of ionospheric disturbances from a few hours to 27 days in advance. These forecasts are supplemental to the long-term predictions, since the occurrence of ionospheric disturbances, which cannot be forecast for long periods in advance, may modify considerably the frequency range within which satisfactory operation can be maintained on a particular circuit. Operating organizations have shown interest in these short‑term forecasts to such an extent that they are now being regularly transmitted by radio at scheduled times.

## 2.3 Working documents for long-term predictions

Recommendation ITU-R P.1240 is the source of basic MUF and optimum working frequency (FOT) for use with predicted 12‑month running mean sunspot numbers *R*12 in making long-term predictions for any part of the world.

# 3 Exchange of basic data used in short-term forecasts

The ISES is a permanent service of the Federations of Astronomical and Geophysical Data Analysis Services (FAGS) under the auspices of the International Union of Radio Science (URSI) in association with the International Astronomical Union (IAU) and the International Union of Geodesy and Geophysics (IUGG).

Within the basic functions of the ISES is the International URSIgram Service which provides standardized rapid free exchange of space weather information and forecasts through its Regional Warning Centres (RWC). In addition, ISES prepares the International Geophysical Calendar (IGC) each year.

At present, there are thirteen Regional Warning Centres scattered around the globe. These centres are located in [Australia (Sydney)](http://www.ips.gov.au/), [Belgium (Brussels)](http://sidc.oma.be), Brazil (Sao Jose dos Campos), [Canada (Ottawa)](http://www.spaceweather.gc.ca/), [China (Beijing)](http://rwcc.bao.ac.cn/), United States of America [(Boulder)](http://www.sec.noaa.gov/index.html), [India (New Delhi)](http://npl-cgc.ernet.in), [Japan (Tokyo)](http://hirweb.crl.go.jp/index.html), [Poland (Warsaw)](http://www.cbk.waw.pl/rwc/rwc.html), [Czech Republic (Prague)](http://rwcprague.ufa.cas.cz/), [Russian](http://www.geospace.ru/) Federation (Moscow), [Sweden (Lund)](http://www.lund.irf.se/) and South Africa (Hermanus). The [European Space Agency (Noordwijk)](http://www.estec.esa.nl/wmwww/wma/spweather/) is a collaborative expert centre providing a venue for data and product exchange for activities in Europe. A data exchange schedule operates with each centre providing and relaying data to the other centres. The centre in Boulder plays a special role as “World Warning Agency”, acting as a hub for data exchange and forecasts.

Further information about ISES can be obtained from their web page at: [www.ises‑spaceweather.org](file:///C:\Users\botha\work\sg3\oct2011\3l\td\111020\www.ises-spaceweather.org).

The WMO space weather portal provides for space weather information about ionospheric storms, geomagnetic storms, radiation storms and solar conditions. Further information about WMO space weather product portal can be obtained from their web page at: <www.wmo.int/pages/prog/sat/spaceweather-productportal_en.php>.