|  |  |  |  |
| --- | --- | --- | --- |
| CZE - Czech Rep. | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Czech Telecommunication Office | Sokolovská 219 P.O. Box 02 225 02 Praha 025 | TF : +420 2 24004647 FAX : +420 2 24004844 EMAIL : sevcikj@ctu.cz |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Brno** | Czech Rep. | TF : +420 5 73385222 FAX : +420 5 73385166 EMAIL : holecp@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 48°58'17''N 016°46'29''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 48°58'17''N 016°46'29''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 48°58'17''N 016°46'29''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 48°58'17''N 016°46'29''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 48°58'17''N 016°46'29''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Ceske Budejovice** | Czech Rep. | TF : +420 3 23605763 FAX : +420 3 23602070 EMAIL : bramboraj@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 49°01'10''N 014°34'58''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°01'10''N 014°34'58''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°01'10''N 014°34'58''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 49°01'10''N 014°34'58''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°01'10''N 014°34'58''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Hradec Králové** | Czech Rep. | TF : +420 5 73385222 FAX : +420 5 73385166 EMAIL : holecp@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 50°06'07''N 015°59'46''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°06'07''N 015°59'46''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°06'07''N 015°59'46''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 50°06'07''N 015°59'46''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°06'07''N 015°59'46''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Jihlava** | Czech Rep. | TF : +420 5 73385222 FAX : +420 5 73385166 EMAIL : holecp@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 49°27'46''N 015°30'27''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°27'46''N 015°30'27''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°27'46''N 015°30'27''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 49°27'46''N 015°30'27''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°27'46''N 015°30'27''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Karlovice** | Karlovice 226 768 43 Kostelec u Holesova Czech Rep. | TF : +420 5 73385222 FAX : +420 5 73385166 EMAIL : holecp@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 49°23'02''N 017°30'58''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |
| 49°23'02''N 017°30'58''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |
| 49°23'02''N 017°30'58''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Fixed man-handled monitoring station.  Multi-element DF antenna with 9 antenna elements. |
| 49°23'02''N 017°30'58''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |
| 49°23'02''N 017°30'58''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Karlovy Vary** | Czech Rep. | TF : +420 3 23605763 FAX : +420 3 23602070 EMAIL : bramboraj@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 50°08'15''N 012°43'45''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°08'15''N 012°43'45''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°08'15''N 012°43'45''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 50°08'15''N 012°43'45''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°08'15''N 012°43'45''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Liberec** | Czech Rep. | TF : +420 3 23605763 FAX : +420 3 23602070 EMAIL : bramboraj@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 50°47'20''N 015°06'21''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°47'20''N 015°06'21''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°47'20''N 015°06'21''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 50°47'20''N 015°06'21''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°47'20''N 015°06'21''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Ostrava** | Czech Rep. | TF : +420 5 73385222 FAX : +420 5 73385166 EMAIL : holecp@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 49°38'07''N 018°29'58''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°38'07''N 018°29'58''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°38'07''N 018°29'58''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 49°38'07''N 018°29'58''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°38'07''N 018°29'58''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Plzen** | Czech Rep. | TF : +420 3 23605763 FAX : +420 3 23602070 EMAIL : bramboraj@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 49°44'43''N 013°26'07''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°44'43''N 013°26'07''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°44'43''N 013°26'07''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 49°44'43''N 013°26'07''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 49°44'43''N 013°26'07''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Praha** | Czech Rep. | TF : +420 3 23605763 FAX : +420 3 23602070 EMAIL : bramboraj@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 50°07'36''N 014°23'05''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled direction-finding station.  Multi-element DF antenna with 9 antenna elements. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Tehov** | Tehov 104 251 01 Ricany u Prahy Czech Rep. | TF : +420 3 23605763 FAX : +420 3 23602070 EMAIL : bramboraj@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 49°58'16''N 014°42'16''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |
| 49°58'16''N 014°42'16''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |
| 49°58'18''N 014°42'18''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Fixed man-handled monitoring station.  Multi-element DF antenna with 9 antenna elements. |
| 49°58'16''N 014°42'16''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |
| 49°58'16''N 014°42'16''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Fixed man-handled monitoring station. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Usti nad Labem** | Czech Rep. | TF : +420 3 23605763 FAX : +420 3 23602070 EMAIL : bramboraj@ctu.cz | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 50°38'48''N 013°38'30''E | Frequency measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°38'48''N 013°38'30''E | Field strength or power flux-density measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°38'48''N 013°38'30''E | Direction-finding measurements | 20 MHz - 1300 MHz | H24 | Remotely controlled monitoring station. |
| 50°38'48''N 013°38'30''E | Bandwidth measurements | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |
| 50°38'48''N 013°38'30''E | Automatic spectrum occupancy surveys | 9 kHz - 3 GHz | H24 | Remotely controlled monitoring station. |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_