|  |
| --- |
| F - France |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Agence Nationale des Fréquences (ANFR) Direction Technique du Contrôle du Spectre | 112, rue Édouard Vaillant94815 Villejuif CedexFrance | TF : +33 1 49583146FAX : +33 1 49583129EMAIL : bcn@anfr.frURL : www.anfr.fr |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Favières (IMS)** | Centre de Contrôle des FréquencesCSTEI FavièresBP 1001928170 FavièresFrance   | TF : +33 2 37385415TF : +33 2 37385392FAX : +33 2 37385418   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 48°32'27''N001°14'03''E | Frequency measurements   | 2 MHz - 30 MHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Rambouillet (IMS)** | Centre de Contrôle International de RambouilletAvenue de Cerqueuse78660 Prunay en YvelinesFrance   | TF : +33 1 34941700FAX : +33 1 34941720   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 48°32'58''N001°47'38''E | Frequency measurements   | 10 kHz - 30 MHz   | H24   | Measurements also carried out by mobile stations (0830-1730).   |
| 48°32'58''N001°47'38''E | Frequency measurements   | 20 MHz - 3 GHz   | H24   | Measurements also carried out by mobile stations (0830-1730).   |
| 48°32'58''N001°47'38''E | Frequency measurements   | 1 GHz - 40 GHz   | 0830-1730   | Measurements also carried out by mobile stations (0830-1730).   |
| 48°32'58''N001°47'38''E | Field strength or power flux-density measurements   | 10 kHz - 30 MHz   | H24   | Measurements also carried out by mobile stations (0830-1730).   |
| 48°32'58''N001°47'38''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0830-1730   | Measurements also carried out by mobile stations (0830-1730).   |
| 48°32'58''N001°47'38''E | Field strength or power flux-density measurements   | 1 GHz - 40 GHz   | 0830-1730   | Measurements also carried out by mobile stations (0830-1730).   |
| 48°32'58''N001°47'38''E | Direction-finding measurements   | 300 kHz - 30 MHz   | H24   | Localization by means of a direction-finding network equipped with Adcock antennas and a single localization station situated at the Rambouillet International Monitoring Center.   |
| 48°32'58''N001°47'38''E | Direction-finding measurements   | 20 MHz - 3 GHz   | H24   | Interferometry.   |
| 48°32'58''N001°47'38''E | Bandwidth measurements   | 10 kHz - 3 GHz   | H24   |   |
| 48°32'58''N001°47'38''E | Bandwidth measurements   | 1 GHz - 40 GHz   | 0830-1730   |   |
| 48°32'58''N001°47'38''E | Automatic spectrum occupancy surveys   | 10 kHz - 30 MHz   | H24   |   |
| 48°32'58''N001°47'38''E | Automatic spectrum occupancy surveys   | 20 kHz - 3 GHz   | H24   |   |
| 48°32'58''N001°47'38''E | Automatic spectrum occupancy surveys   | 1 GHz - 40 GHz   | 0830-1730   |   |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_