|  |  |  |  |
| --- | --- | --- | --- |
| G - United Kingdom | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Ofcom | Ofcom Riverside House 2a Southwark Bridge Road London SE1 9HA | PHONE: +44 20 79813109 TELEFAX: +44 20 79813208 EMAIL: ifc.enquiries@ofcom.org.uk | Ofcom Spectrum Management Center (SMC) is staffed 24 hours - 365 days. |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Baldock (IMS)** | Royston Road Baldock Hertfordshire SG7 6SH United Kingdom | PHONE: +44 1462 428528 EMAIL: smc@ofcom.org.uk | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 52°00'00"N 000°08'00"W | Frequency measurements | 10 kHz - 1 GHz | H24 | Measurements on A1A, A3E, F1B, F3E, G1D, G7D, J7B and D7W. |
| 52°00'00"N 000°08'00"W | Field strength or power flux-density measurements | 10 kHz - 240 kHz | H24 |  |
| 52°00'00"N 000°08'00"W | Direction-finding measurements | 100 kHz - 30 MHz | H24 | Better than ± 0.5 degrees dependant on the signal to noise ratio of the wanted signal.  MF/HF Super Resolution DF ECopy. This DF has 3 switchable arrays (MF, low HF and high HF) to cover the 100 kHz to 30 MHz band. |
| 52°00'00"N 000°08'00"W | Frequency measurements | 1 GHz - 3 GHz | H24 | Measurements on A1A, A3E, F1B, F3E, G1D, G7D, J7B and D7W. |
| 52°00'00"N 000°08'00"W | Field strength or power flux-density measurements | 240 kHz - 30 MHz | H24 |  |
| 52°00'00"N 000°08'00"W | Field strength or power flux-density measurements | 30 MHz - 3 GHz | H24 |  |
| 52°00'00"N 000°08'00"W | Bandwidth measurements | 10 kHz - 3 GHz | H24 | ~~E~~lectronic results available upon request. |
| 52°00'00"N 000°08'00"W | Automatic spectrum occupancy surveys | 10 kHz - 3 GHz | H24 | ~~E~~lectronic results available upon request. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Fife** | Ofcom Royston Road Baldock Hertfordshire SG7 6SH United Kingdom | PHONE: +44 1462 428528 EMAIL: smc@ofcom.org.uk | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 56°16'05"N 002°48'47"W | Direction-finding measurements | 100 kHz - 30 MHz | H24 | Better than ± 0.5 degrees dependant on the signal to noise ratio of the wanted signal.  MF/HF Super Resolution DF ECopy.  Remotely controlled from Baldock, Hertfordshire. |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_