|  |
| --- |
| KEN - Kenya |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| National Spectrum Control CentreOffice of the DirectorFrequency Spectrum ManagementCommunications Authority Commission of Kenya | Waiyaki WayP.O. Box 1444800800 Nairobi | TF : +254 20 4242000TF : +254 70 3042000EMAIL : info@ca.go.ke |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Eldoret**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 00°28'54''N035°16'29''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°28'54''N035°16'29''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°28'54''N035°16'29''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | DF omni-vertical antenna.Remotely operated station.   |
| 00°28'54''N035°16'29''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°28'54''N035°16'29''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Garissa**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 20 4242000TF : +254 70 3042000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 00°22'28''S039°42'56''E | Frequency measurements   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 00°22'28''S039°42'56''E | Field strength or power flux-density measurements   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 00°22'28''S039°42'56''E | Direction-finding measurements   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 00°22'28''S039°42'56''E | Bandwidth measurements   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 00°22'28''S039°42'56''E | Automatic spectrum occupancy surveys   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Kabete**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 20 4242000TF : +254 70 3042000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 01°15'45''S036°45'29''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Manned station.   |
| 01°15'45''S036°45'29''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Manned station.   |
| 01°15'45''S036°45'29''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | Manned station.   |
| 01°15'45''S036°45'29''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Manned station.   |
| 01°15'45''S036°45'29''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Manned station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Kahawa**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 01°12'53''S036°56'50''E | Frequency measurements   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Field strength or power flux-density measurements   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Bandwidth measurements   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Automatic spectrum occupancy surveys   | 9 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 01°12'53''S036°56'50''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Kisumu**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 00°03'24''S034°45'20''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°03'24''S034°45'20''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°03'24''S034°45'20''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | DF omni-vertical antenna.Remotely operated station.   |
| 00°03'24''S034°45'20''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°03'24''S034°45'20''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Kitale**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 20 4242000TF : +254 70 3042000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 01°02'35''N032°52'12''E | Frequency measurements   | 10 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 01°02'35''N032°52'12''E | Field strength or power flux-density measurements   | 10 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 01°02'35''N032°52'12''E | Bandwidth measurements   | 10 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |
| 01°02'35''N032°52'12''E | Automatic spectrum occupancy surveys   | 10 kHz - 30 MHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Mazeras**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 03°58'25''S039°32'48''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 03°58'25''S039°32'48''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 03°58'25''S039°32'48''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 03°58'25''S039°32'48''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 03°58'25''S039°32'48''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Mobile station**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
|   | Frequency measurements   | 20 MHz - 6 GHz   | 0800-1700   | Four mobile units.   |
|   | Field strength or power flux-density measurements   | 20 MHz - 6 GHz   | 0800-1700   | Four mobile units.   |
|   | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | DF omni-vertical antenna.Four mobile units.   |
|   | Bandwidth measurements   | 20 MHz - 6 GHz   | 0800-1700   | Four mobile units.   |
|   | Automatic spectrum occupancy surveys   | 20 MHz - 6 GHz   | 0800-1700   | Four mobile units.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Mombasa City**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 04°04'50''S040°40'24''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 04°04'50''S040°40'24''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 04°04'50''S040°40'24''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | DF omni-vertical antenna.Remotely operated station.   |
| 04°04'50''S040°40'24''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 04°04'50''S040°40'24''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Nakuru**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 00°17'31''S036°07'33''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°17'31''S036°07'33''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°17'31''S036°07'33''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | DF omni-vertical antenna.Remotely operated station.   |
| 00°17'31''S036°07'33''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 00°17'31''S036°07'33''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Railways**  | Waiyaki WayP.O. Box 14448Nairobi 00800Kenya   | TF : +254 70 3042000TF : +254 20 4242000EMAIL : info@ca.go.ke   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 01°18'53''S036°50'32''E | Frequency measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 01°18'53''S036°50'32''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 01°18'53''S036°50'32''E | Direction-finding measurements   | 20 MHz - 3 GHz   | 0800-1700   | DF omni-vertical antenna.Remotely operated station.   |
| 01°18'53''S036°50'32''E | Bandwidth measurements   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |
| 01°18'53''S036°50'32''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | 0800-1700   | Remotely operated station.   |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_