|  |
| --- |
| SEN - Senegal |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Autorité de Régulation des Télécommunications et des Postes | B.P. 14130Dakar Peytavin | TF : +221 33 8690369FAX : +221 33 8690370EMAIL : abdou.ndiaye@artp.snEMAIL : contact@artp.sn |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Khombole**  | ARTPCentre de contrôle de KhomboleKhomboleSénégal   | TF : +221 33 8690369FAX : +221 33 8690370EMAIL : contact@artp.sn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 14°45'20''N016°42'11''W | Frequency measurements   | 3 MHz - 30 MHz   | H24   |   |
| 14°45'20''N016°42'11''W | Field strength or power flux-density measurements   | 3 MHz - 30 MHz   | H24   |   |
| 14°45'20''N016°42'11''W | Direction-finding measurements   | 3 MHz - 30 MHz   | H24   |   |
| 14°45'20''N016°42'11''W | Bandwidth measurements   | 3 MHz - 30 MHz   | H24   |   |
| 14°45'20''N016°42'11''W | Automatic spectrum occupancy surveys   | 3 MHz - 30 MHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Yeumbeul**  | ARTPCentre de Contrôle de YeumbeulYeumbeulSénégal   | TF : +221 33 8690369FAX : +221 33 8690370EMAIL : contact@artp.sn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 14°47'09''N017°20'08''W | Frequency measurements   | 30 MHz - 3 GHz   | HX   |   |
| 14°47'09''N017°20'08''W | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   | HX   |   |
| 14°47'09''N017°20'08''W | Direction-finding measurements   | 30 MHz - 3 GHz   | HX   | Log-periodic antenna.MF/HF: wire antenna.Biconical (umbrella) antenna.Parabolic antenna.   |
| 14°47'09''N017°20'08''W | Bandwidth measurements   | 30 MHz - 3 GHz   | HX   |   |
| 14°47'09''N017°20'08''W | Automatic spectrum occupancy surveys   | 30 MHz - 3 GHz   | HX   |   |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_