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1. Abstract

This contribution proposes few definitions for NGN. 
2. Discussion

In both working groups 2 and 6 there are terms which have been used in some documents but with no clear definition. So, it is important that there is a clear definition of each term to help better understanding. For this reason the following terms are proposed. 
3. Proposal

It is proposed to accept the following terms and place them in [1] or [2] as appropriate.

Application: A structured set of capabilities, which provide value-added functionality supported by one or more services, which requires information to be passed across an API interface.

Call server: An entity that acts both as a server and a client. It provides address translation for the purpose of making requests on behalf of other clients.  It also ensures that a request is sent to another entity by enforcing specific call admission control policies. A call server is sometimes called a “gatekeeper” in some specifications

Customer network: A telecommunications network belonging to the customer and located in the customer premise(s). The customer network is connected to the user side of an access network.  

Node: A network element (switch, router, exchange) providing switching and/or routing capabilities.

NGphone: The NGphone (Next Generation phone) is an assembly of apparatus for telephony including at least a microphone, a receiver, a dialler, an alerter, an optional video camera and/or monitor, and related applications permitting the establishment of a communication in both directions between two parties (e.g. using SIP applications and a headset). It may be implemented in standalone hardware or as a software application.
Service: A structured set of telecommunication capabilities intended to support applications or requirements for telecommunication services.
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