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1. Problem description

This contribution addresses authentication for subscribers making use of Wi-Fi or LAN access connection in network domains operated by other operators.

As it is unclear that full Mobility with in call handover can be made available in NGN release 1 it is proposed to make authentication data available to other network domains in this release.

It is suggested that any roaming mechanism is aligned with Mobility as implemented by 3GPP release 6. This will allow roaming users using e.g. Wi-Fi or LAN access to connect to the visited network without further registration with the local network operator.

2.  Proposals

In the “draft technical specification NGN Security Framework” (FGNGN-OD-0002R1) 
section 9.2 “Network domain security” add the requirement to make user authentication data available to other network domains in NGN release 1 for the purpose of supporting roaming on Wi-Fi and LAN access connections.
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