David Barrett

Chairman SG 6 Rapporteur Group on spectrum requirements   
for the future of the broadcasting Service

Questionnaire on spectrum requirements for the future  
of sound and television broadcasting

|  |  |
| --- | --- |
| **Name of the Administration:** | State Communication Agency under the Government of the Kyrgyz Republic |
| **Contact person:** | **Kudaibergenov Islam** |
| E-mail address: | [*nta@infotel.kg*](mailto:nta@infotel.kg),[*ikudaibergenov92@gmail.com*](mailto:ikudaibergenov92@gmail.com) |
| Telephone number: | *+996 (312) 548 298* |

|  |  |
| --- | --- |
| **Name of the Sector Member:** |  |
| **Contact person:** |  |
| E-mail address: |  |
| Telephone number: |  |
| **What best describes your organisation?**  Commercial broadcaster/Public service broadcaster/ Service provider/ Other (please describe) |  |
| **The geographical area over which you operate:** |  |

SECTION ONE – Television broadcasting

1) a) Is your country still using analogue television?

b) If yes, has analogue television switch-off commenced?

c) If your country has any plans to switch-off analogue television.

i) When is the analogue switch-off process expected to be completed?

ii) How much extra spectrum will be required during the transition phase to digital terrestrial television broadcasting?

**Reply: a) Yes.**

**b) No.**

**c) Nowadays the administration of the Kyrgyz Republic developing the**

**concept of analogue switch-off of television.**

2) a) Please indicate how many analogue television transmitters are in operation in your country and in which bands.

b) What channel bandwidths are used for analogue television?

c) What is the spectrum requirement for analogue television in your country?

A proposed format for responses to question 2a) and 2b) is provided in Annex 1

**Reply: responses to questions 2a) and 2b) are provided in Annex 1**

**c) Spectrum requirement for analogue television in our country is 320 MHz**

3) a) What is the percentage of viewer uptake of terrestrial television in your country?

b) If possible, please also provide details of the number or proportion of users who receive television primarily by terrestrial means by:

i) Fixed roof top antenna, or  
ii) Portable indoor antenna.

**Reply: a) 99.4 %**

**b) Such information is missing**

4) If your country has switched or is considering switching to digital terrestrial television broadcasting

a) What system standard is your country using or considering adopting   
(as specified in Recommendations ITU-R BT.1306 and BT.1877)?

b) When did your country start or when is it proposing to start the introduction of digital terrestrial television services?

c) Please provide further detail on the number of multiplexes in use, their technical specifications, the percentage of geographic area or population they cover or are intended to cover and the total spectrum use.

A proposed format for detailed responses is provided in Annex 2

**Reply: Responses to questions are provided in Annex 2**

5) a) What frequencies/channels are currently used or intended to be used by digital terrestrial television broadcasting in your country? Please distinguish between those in use and those intended to be used?

b) Please indicate how many digital terrestrial television transmitters are currently used or intended to be used and in which bands.

c) What channel bandwidth is used or intended to be used for digital terrestrial television in your country?

A proposed format for responses to question 5b) and 5c) is provided in Annex 1

**Reply: a) Frequencies/channels in the frequency range 470 – 790 MHz are currently used by digital terrestrial television broadcasting.**

**Responses to questions 5b) and 5c) are provided in Annex 1**

6) a) Are the terrestrial television frequency bands also shared with other primary services in your country?

b) If yes, please give details of those systems and their spectrum use.

**Reply: a) No**

7) a) Are the terrestrial television frequency bands also shared with secondary services used for the support of broadcasting such as SAB/SAP (services ancillary to broadcasting/production), or other types of services such as radio astronomy or wind-profile radar?

b) If yes, please give details of those systems and their spectrum use.

**Reply: a) No**

8) a) Does your country foresee a requirement for new and enhanced services, including multimedia and data applications, HD, 3D, and UHD television, on the terrestrial television platform?

b) If yes, please give indicative details of the number and nature of services planned, and if known, the expected timeframe for their introduction.

**Reply: a) Introduction of HD and 3D television is considered in the future**

**b) Such information is missing**

9) a) Are there plans in your country to launch more multiplexes in the future?

b) If yes, how many more and when? Please also indicate the expected timeframe for their introduction.

**Reply: a) Yes**

**] b) In the future our country will launch 4 multiplexes**

10) a) What is the amount of spectrum your country foresees will be required for terrestrial television broadcasting, taking into consideration the responses to Questions 5, 6, 7, 8, and 9? Please indicate the modes of transmission that will be used, and timeframes.

**Reply: Our country foresees to use 320 MHz for terrestrial broadcasting in the frequency range 470 – 790 MHz in transmission mode DVB-T2/MPEG-4/OFDM**

SECTION TWO – Sound broadcasting

11) a) What analogue sound broadcasting standards are used in your country and what bands are they operating in?

b) Please indicate how many analogue radio transmitters are in operation in your country and in which bands.

c) What channel bandwidths do they use?

A proposed format for responses to question 11b) and 11c) is provided in Annex 1

**Reply: a) analogue sound broadcasting standard - D/SECAM in the frequency range 87.5 – 108 MHz is used in our country**

**Responses to questions 11b) and 11c) are provided in Annex 1**

12) a) Is additional spectrum required for growth in the analogue sound broadcasting platform in your country?

b) If yes, how much additional spectrum is required?

**Reply: a) No**

13) a) Is your country considering introducing, or has it already introduced digital sound broadcasting?

b) If yes, which system standards are used or are being considered for adoption (as specified in Recommendations ITU-R BS.1114, BS.1514, BS.1615)?

c) When did your country start or when does it propose to start digital sound broadcasting?

d) What channel bandwidths is your country using or considering using?

e) What frequencies are currently used or intended to be used by digital sound broadcasting in your country? Please distinguish between those in use and those intended to be used.

f) What is the percentage of the population that is covered by digital sound broadcasting by direct reception in your country?

g) What additional spectrum was required or is considered to be required for the transition to digital sound broadcasting?

h) Please indicate how many digital radio transmitters are currently used or intended to be used and in which bands.

i) What is the spectrum requirement for digital sound broadcasting in your country?

j) If your country has introduced digital sound broadcasting, how long will it continue to use analogue sound broadcasting?

A proposed format for responses to question 13d) and 13h) is provided in Annex 1

**Reply: No**

14) a) Are the terrestrial sound broadcasting bands also shared with other primary services in your country?

b) If yes, please give details of those systems and their spectrum use.

**Reply: No**

15) a) Are the terrestrial sound broadcasting bands also shared with secondary services e.g., used for the support of broadcasting such as SAB/SAP (services ancillary to broadcasting/production), or other types of services such as radio astronomy or wind-profile radar?

b) If yes, please give details of those systems and their spectrum use.

**Reply: No**

16) a) What is the amount of spectrum your country foresees will be required for terrestrial sound broadcasting, taking into consideration the responses to the previous questions? Please indicate the modes of transmission that will be used, and timeframes.

**Reply: Our country nowadays to use 22 MHz for аanalogue sound broadcasting in the frequency range 87,5 – 108 MHz.**

SECTION THREE –Multimedia broadcasting

17) a) Is your country considering introducing or has already introduced multimedia broadcasting?

b) If yes which system standards is your country using or considering using (as specified in Recommendations ITU-R BT.1833 and BT.2016)?

c) In which Bands?

d) When did your country start or when does it propose to start digital multimedia broadcasting?

e) What are the current and proposed population coverages for digital multimedia broadcasting in your country?

f) What is the spectrum requirement for multimedia broadcasting in your country?

g) If your country has introduced digital multimedia broadcasting, please provide further information to describe the system, its implementation and any limitations on its operation.

**Reply: 17) Introduction of multimedia broadcasting is considered in the future.**

**Such information about questions b) c) d) e) f) g) are missing.**

ANNEX 1 tO attachment 1

Suggested form of presentation of reply to Questions 2, 5, 11, and 13:

A sample response is shown in *Italics* for guidance only.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Country** | **Band** | | **Number of Transmitting Stations\*** | | | |
| **Analogue Radio**)(Q11b & Q11c) | **Digital Radio** (Q13d & Q13h) | **Analogue TV** (Q2a & Q2)b | **Digital TV** (Q5b & Q5c) |
| **Channel bandwidth (MHz)** | | *VHF I 180kHz*  *VHF II 300kHz* |  | *8MHz* | *8MHz* |
| **Kyrgyz Republic** | **LF** | 148.5-283.5 kHz |  |  |  |  |
| **MF** | 525-526.5 kHz |  |  |  |  |
| **MF** | 526.5-1606.5 kHz  1606.5-1705 kHz | 23 |  |  |  |
| **MF** |  |  |  |
| **HF** | 2.3-26.1 MHz\*\* |  |  |  |  |
| **VHF I** | 47-50 MHz | 25 |  |  |  |
| 50-54 MHz |  |  |  |
| 54-68 MHz |  |  |  |
| 68-72 MHz |  |  |  |
| 76-87.5 MHz |  |  |  |
| **VHF II** | 87.5-108 MHz | 343 |  |  |  |
| **VHF III** | 174-216 MHz |  |  | 450 |  |
| **VHF III** | 216-230 MHz |  |  |  |
| **UHF IV** | 470-790 MHz |  |  | 345 | 41 |
| **UHF V** |  |  |
| **UHF V** | 790-890 MHz |  |  |  |  |
| **UHF V** | 890-960 MHz |  |  |  |  |
|  | 1452-1492 MHz |  |  |  |  |
|  | 11.7-12.5 GHz |  |  |  |  |
|  | 12.5-12.7 GHz |  |  |  |  |
|  | 40.5-42.5 GHz |  |  |  |  |
|  | 74-76 GHz |  |  |  |  |
| \* Transmitting stations please include “main stations” and “relay stations.” Please use parenthesis to indicate stations that have still to be brought into use  \*\* The bands 3900-3950D, 3950-4000D kHz; the bands for tropical broadcasting: 2300-2498, 3200-3400D, 4750-4995 D, 5005-5060D kHz and the Article 12 Bands 5 900-5 950D, 5 950-6 200, 7 200-7 300, 7 300-7 400D, 7 400-7 450, 9 400-9 500D, 9 500-9 900, 11 600-11 650D, 11 650-12 050, 12 050-12 100D, 13 570-13 600D, 13 600-13 800, 13 800-13 870D, 15 100-15 600, 15 600-15 800D, 17 480-17 550D, 17 550-17 900, 18 900-19 020D, 21 450-21 850, 25 670-26 100.  D Resolution 517 (Rev.WRC-07) applies. In the HF bands subject to Article 12 see also No. 5.134. | | | | | | |

ANNEX 2 TO ATTACHMENT 1

Suggested form of presentation of reply to Question 4: *If your country has switched or is considering switching to digital terrestrial television broadcasting, what system standards is it using or considering adopting? When did your country start, or when is it proposed to start the introduction of digital terrestrial television services? Please provide further detail on the number of multiplexes in use, their technical specifications, the percentage of geographic area or population they cover or are intended to cover and the total spectrum use.*

A sample response is shown in *italics* for guidance only.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Country** | **No of multi-plexes** | **System & modulation** | **FEC** | **GI** | **Reception mode[[1]](#footnote-1)** | **Capacity per multiplex (Mb/s)** | **Current percentage population coverage** | **Intended percentage population coverage** | **Content per multiplex** | **Total capacity (Mb/s)** | **Total spectrum bandwidth used or intended for implementation (MHz)** | **Any additional comments (e.g. duration of licences)** |
| **Kyrgyz Republic** | *12* | *DVB-T, 64-QAM* | *¾* | *1/16* | *Fixed* |  | *7.99%* | *7.99%* | *8 SD MPEG2* |  | *320* |  |
| *4* | *DVB-T2, 256-QAM* | *¾* | *1/4* | *Fixed* |  | *58.9%* | *93,24 %* | *8 SD MPEG4* |  | *320* |  |

1. [↑](#footnote-ref-1)