|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 7 toDocument 32(Add.21)-E** |
|  | **29 September 2015** |
|  | **Original: English** |
|  |
| Asia-Pacific Telecommunity Common Proposals |
| Proposals for the work of the conference |
|  |
| Agenda item 7(G) |

7 to consider possible changes, and other options, in response to Resolution 86 (Rev. Marrakesh, 2002) of the Plenipotentiary Conference, an advance publication, coordination, notification and recording procedures for frequency assignments pertaining to satellite networks, in accordance with Resolution **86 (Rev.WRC‑07)** to facilitate rational, efficient, and economical use of radio frequencies and any associated orbits, including the geostationary‑satellite orbit;

7(G) Issue G – Clarification of bringing into use information provided under RR Nos. **11.44**/**11.44B**

Introduction

APT Members support the single Method G, with its proposed regulatory text, as it was added to the CPM Report.

Proposals

ARTICLE 11

Notification and recording of frequency
assignments1, 2, 3, 4, 5, 6, 7, 7*bis*    (WRC‑12)

Section II − Examination of notices and recording of frequency assignments
in the Master Register

MOD ASP/32A21A7/1

11.44 The notified date20, 21, ADD 21*bis* of bringing into use of any frequency assignment to a space station of a satellite network shall be not later than seven years following the date of receipt by the Bureau of the relevant complete information under No. 9.1 or 9.2, as appropriate. Any frequency assignment not brought into use within the required period shall be cancelled by the Bureau after having informed the administration at least three months before the expiry of this period.  (WRC‑15)

MOD ASP/32A21A7/2

11.44B A frequency assignment to a space station in the geostationary-satellite orbit shall be considered as having been brought into use when a space station in the geostationary-satellite orbit with the capability of transmitting or receiving that frequency assignment has been deployed and maintained at the notified orbital position for a continuous period of ninety days. The notifying administration shall so inform the Bureau within thirty days from the end of the ninety-day periodADD 21*bis*.    (WRC‑15)

ADD ASP/32A21A7/3

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

21*bis*  11.44.3 and 11.44B.1 Upon receipt of this information, and whenever it appears from reliable information available that a notified assignment has not been brought into use in accordance with Nos. **11.44** and/or **11.44B**, as the case may be, the consultation procedures and the subsequent applicable course of action prescribed in No. **13.6** shall apply, as appropriate.     (WRC‑15)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_