|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15) Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Document 80-E** |
|  | **19 October 2015** |
|  | **Original: English** |
|  | |
| Greece | |
| Proposals for the work of the conference | |
|  | |
| Agenda item 8 | |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC‑07)**;

Introduction

In accordance with Resolution 26 (Rev.WRC-07) the Greek Administration has reviewed the footnotes to the Table of Frequency Allocations in Article 5 of the Radio Regulations and proposes:

1) to delete footnote No. 5.315, due to the fact that the spectrum band 790-862 MHz has been awarded to mobile electronic communication service providers and the spectrum band 790-838 MHz is no longer being used by the broadcasting service;

2) to delete its country name from footnote No. 5.359, due to the fact that according to the National Frequency Register there aren’t any rights of use in the frequency bands 1 550-1 559 MHz and 1 610-1 660 MHz for fixed service applications nor are there any intentions to use these bands for fixed service in the future;

3) to delete its country name from footnote No. 5.506B, since new systems are planned to be developed in Greece and ITU procedures will be applied.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

SUP GRC/80/1

5.315 *Alternative allocation:*  in Greece, the band 790-838 MHz is allocated to the broadcasting service on a primary basis.    (WRC‑12)

MOD GRC/80/2

5.359 *Additional allocation:* in Germany, Saudi Arabia, Armenia, Austria, Azerbaijan, Belarus, Benin, Cameroon, the Russian Federation, France, Georgia, Guinea, Guinea-Bissau, Jordan, Kazakhstan, Kuwait, Lithuania, Mauritania, Uganda, Uzbekistan, Pakistan, Poland, the Syrian Arab Republic, Kyrgyzstan, the Dem. People’s Rep. of Korea, Romania, Tajikistan, Tanzania, Tunisia, Turkmenistan and Ukraine, the bands 1 550-1 559 MHz, 1 610-1 645.5 MHz and 1 646.5-1 660 MHz are also allocated to the fixed service on a primary basis. Administrations are urged to make all practicable efforts to avoid the implementation of new fixed-service stations in these bands.    (WRC‑15)

MOD GRC/80/3

5.506B Earth stations located on board vessels communicating with space stations in the fixed-satellite service may operate in the frequency band 14-14.5 GHz without the need for prior agreement from Cyprus and Malta, within the minimum distance given in Resolution **902 (WRC‑03)** from these countries.     (WRC-15)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_