|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 1 toDocument 82-E** |
|  | **16 October 2015** |
|  | **Original: English** |
|  |
| Uganda (Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 1.1 |

1.1 to consider additional spectrum allocations to the mobile service on a primary basis and identification of additional frequency bands for International Mobile Telecommunications (IMT) and related regulatory provisions, to facilitate the development of terrestrial mobile broadband applications, in accordance with Resolution **233 (WRC‑12)**;

Introduction

This document provides position of Uganda for candidate band 3 400-3 600 MHz.

Uganda’s position for the mentioned candidate band is Method A – No change.

Proposal

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

NOC UGA/82A1/1

2 700-4 800 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 3 400-3 600FIXEDFIXED-SATELLITE(space-to-Earth)Mobile 5.430ARadiolocation5.431 | 3 400-3 500FIXEDFIXED-SATELLITE (space-to-Earth)AmateurMobile 5.431ARadiolocation 5.4335.282 | 3 400-3 500FIXEDFIXED-SATELLITE (space-to-Earth)AmateurMobile 5.432BRadiolocation 5.4335.282 5.432 5.432A |
| 3 500-3 700FIXEDFIXED-SATELLITE (space-to-Earth)MOBILE except aeronautical mobileRadiolocation 5.433 | 3 500-3 600FIXEDFIXED-SATELLITE (space-to-Earth)MOBILE except aeronautical mobile 5.433ARadiolocation 5.433 |

**Reasons:** Whereas there are existing WiMax services for the band and this band has already been identified/allocated to MS for IMT as per in footnotes (RR Nos. 5.430A, 5.432A, 5.432B), there are *compatibility issues between IMT and this band as per the CPM text and furthermore previous cases of interference have been reported between wireless technologies such as WiMAX and C band.*

\_\_\_\_\_\_\_\_\_\_\_\_\_\_