|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 22 toDocument 132-E** |
|  | **19 October 2015** |
|  | **Original: English** |
|  |
| United Kingdom of Great Britain and Northern Ireland |
| Proposals for the work of the conference |
|  |
| Agenda item 8 |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC‑07)**;

Introduction

The United Kingdom (UK) administration has reviewed the footnotes which include explicit references to the “United Kingdom”.

We therefore make the following proposals for specific footnotes where UK is referenced. It should be noted that the UK is party to other regional contributions which amend footnotes which may have the UK referenced. This contribution should therefore be viewed alongside those proposals and the changes here do not impact, replicate nor contradict those potential changes.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD G/132A22/1

5.314 *Additional allocation*:  in Austria, Italy, Moldova, Uzbekistan and Kyrgyzstan, the band 790-862 MHz is also allocated to the land mobile service on a secondary basis.     (WRC‑15)

**Reasons:** The frequency band 790-862 MHz is allocated to mobile (except aeronautical mobile) on a primary basis in Region 1, therefore this footnote seems superfluous and therefore the UK can be removed.

MOD G/132A22/2

5.316 *Additional allocation:*  in Germany, Saudi Arabia, Bosnia and Herzegovina, Burkina Faso, Cameroon, Côte d'Ivoire, Croatia, Denmark, Egypt, Finland, Greece, Israel, Jordan, Kenya, Libya, The Former Yugoslav Republic of Macedonia, Liechtenstein, Mali, Monaco, Montenegro, Norway, the Netherlands, Portugal, the Syrian Arab Republic, Serbia, Sweden and Switzerland, the band 790-830 MHz, and in these same countries and in Spain, France, Gabon and Malta, the band 830-862 MHz, are also allocated to the mobile, except aeronautical mobile, service on a primary basis. However, stations of the mobile service in the countries mentioned in connection with each band referred to in this footnote shall not cause harmful interference to, or claim protection from, stations of services operating in accordance with the Table in countries other than those mentioned in connection with the band. This allocation is effective until 16 June 2015.     (WRC‑15)

**Reasons:** In Region 1 the frequency band 790-862 MHz is allocated to the mobile (except aeronautical mobile) on a primary basis. Therefore this footnote seems superfluous and therefore the UK can be removed. It is noted that this footnote has an effective end date of 16 June 2015.

MOD G/132A22/3

5.431 *Additional allocation:*in Germany and Israel, the band 3 400-3 475 MHz is also allocated to the amateur service on a secondary basis.     (WRC-15)

**Reasons:** Changes in the UK frequency allocations means that this footnote should no longer reference the UK.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_