|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| COMMITTEE 4 | **Document 156-E** |
|  | **3 November 2015** |
| Source: Document DT/26 | **Original: English** |
|  |
| Chairman, Working Group 4B |
| First report of Working Group 4B to Committee 4 on agenda item 1.15 |
|  |
| Agenda item 1.15 |

1.15 to consider spectrum demands for on-board communication stations in the maritime mobile service in accordance with Resolution **358 (WRC‑12)**;

|  |  |
| --- | --- |
| **Title** | **Agenda item** |
| Article 5 | 1.15 |

 M.A. EL-MOGHAZI

Chairman, Working Group 4B

Office: 232 (CICG)

 Email: WG4Bwrc15@itu.int

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD WG4B/156/1#30255

410-460 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 456-459 FIXED MOBILE 5.286AA 5.271 MOD 5.287 5.288  |

MOD WG4B/156/2#30256

460-890 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 460-470 FIXED MOBILE 5.286AA Meteorological-satellite (space-to-Earth)  MOD 5.287 5.288 5.289 5.290 |

MOD WG4B/156/3#30257

5.287 Use of the frequency bands 457.5125-457.5875 MHz and 467.5125-467.5875 MHz by the maritime mobile service is limited to on-board communication stations. The characteristics of the equipment and the channelling arrangement shall be in conformity with Recommendation ITU‑R M.1174‑3. The use of these frequency bands in territorial waters is subject to the national regulations of the administration concerned.     (WRC‑15)

SUP WG4B/156/4#30258

RESOLUTION 358 (WRC‑12)

Consideration of improvement and expansion of on-board communication stations in the maritime mobile service in the UHF bands

\_\_\_\_\_\_\_\_\_\_\_\_\_\_