|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 7 toDocument 12(Add.19)-E** |
|  | **25 June 2019** |
|  | **Original: Russian** |
|  |
| Regional Commonwealth in the field of Communications Common Proposals |
| proposals for the work of the conference |
|  |
| Agenda item 7(G) |

7 to consider possible changes, and other options, in response to Resolution 86 (Rev. Marrakesh, 2002) of the Plenipotentiary Conference, an advance publication, coordination, notification and recording procedures for frequency assignments pertaining to satellite networks, in accordance with Resolution **86 (Rev.WRC-07)**, in order to facilitate rational, efficient and economical use of radio frequencies and any associated orbits, including the geostationary-satellite orbit;

7(G) Issue G - Updating the reference situation for Regions 1 and 3 networks under RR Appendices **30** and **30A** when provisionally recorded assignments are converted into definitive recorded assignments

Introduction

The RCC Administrations consider it unreasonable to modify § **4.1.18** of RR Appendices **30** and **30A** whereby the reference situation of the “interfered-with” satellite network would be updated only after agreement between the Administration notifying that network and the Administration notifying the new “interfering network” (Method G3).

APPENDIX 30 (REV.WRC‑15)[[1]](#footnote-1)\*

Provisions for all services and associated Plans and List[[2]](#footnote-2)1 for
the broadcasting-satellite service in the frequency bands
11.7-12.2 GHz (in Region 3), 11.7-12.5 GHz (in Region 1)
         and 12.2-12.7 GHz (in Region 2)    (WRC‑03)

ARTICLE 4     (Rev.WRC‑15)

Procedures for modifications to the Region 2 Plan or
for additional uses in Regions 1 and 3[[3]](#footnote-3)3

## 4.1 Provisions applicable to Regions 1 and 3

NOC RCC/12A19A7/1

4.1.18 If, in spite of the application of § 4.1.16 and 4.1.17, there is still continuing disagreement and the assignment which was the basis of the disagreement is not an assignment in the Regions 1 and 3 Plan, or in the Region 2 Plan or for which the procedure of § 4.2 has been initiated, and if the notifying administration insists that the proposed assignment be included in the Regions 1 and 3 List, the Bureau shall provisionally enter the assignment in the Regions 1 and 3 List with an indication of those administrations whose assignments were the basis of the disagreement; however, the entry shall be changed from provisional to definitive recording in the List only if the Bureau is informed that the new assignment in the Regions 1 and 3 List has been in use, together with the assignment which was the basis for the disagreement, for at least four months without any complaint of harmful interference being made.     (WRC‑03)

**Reasons:** Given the complexity of reaching agreement in a number of cases and the consequent difficulties in converting provisionally recorded frequency assignments into definitive recorded assignments, the existing procedure of recording on the basis of four months of interference-free operation should be maintained.

NOC RCC/12A19A7/2

4.1.18*bis* When requesting the application of § 4.1.18, the notifying administration shall undertake to meet the requirements of § 4.1.20 and provide to the administration in respect of which § 4.1.18 is applied, with a copy to the Bureau, a description of the steps by which it undertakes to meet these requirements. Once an assignment is entered in the List provisionally under the provisions of § 4.1.18, the calculation of the equivalent protection margin (EPM)[[4]](#footnote-4)9 of an assignment in the Regions 1 and 3 List or for which the procedure of Article 4 has been initiated and which was the basis for the disagreement shall not take into account the interference produced by the assignment for which the provisions of § 4.1.18 have been applied.     (WRC‑03)

**Reasons:** Given the complexity of reaching agreement in a number of cases and the consequent difficulties in converting provisionally recorded frequency assignments into definitive recorded assignments, the existing procedure of recording on the basis of four months of interference-free operation should be maintained.

APPENDIX 30A (REV.WRC‑15)[[5]](#footnote-5)\*

Provisions and associated Plans and List[[6]](#footnote-6)1 for feeder links for the broadcasting-satellite service (11.7-12.5 GHz in Region 1, 12.2-12.7 GHz
in Region 2 and 11.7-12.2 GHz in Region 3) in the frequency bands
14.5-14.8 GHz[[7]](#footnote-7)2 and 17.3-18.1 GHz in Regions 1 and 3,
and 17.3-17.8 GHz in Region 2     (WRC‑03)

ARTICLE 4     (Rev.WRC‑15)

Procedures for modifications to the Region 2 feeder-link Plan
or for additional uses in Regions 1 and 3

## 4.1 Provisions applicable to Regions 1 and 3

NOC RCC/12A19A7/3

4.1.18 If, in spite of the application of § 4.1.16 and 4.1.17, there is still continuing disagreement and the assignment which was the basis of the disagreement is not an assignment in the Regions 1 and 3 Plan, or in the Region 2 Plan or for which the procedure of § 4.2 has been initiated, and if the notifying administration insists that the proposed assignment be included in the Regions 1 and 3 feeder-link List, the Bureau shall provisionally enter the assignment in the Regions 1 and 3 feeder-link List with an indication of those administrations whose assignments were the basis of the disagreement; however, the entry shall be changed from provisional to definitive recording in the feeder-link List only if the Bureau is informed that the new assignment in the Regions 1 and 3 feeder-link List has been in use, together with the assignment which was the basis for the disagreement, for at least four months without any complaint of harmful interference being made.     (WRC‑03)

**Reasons:** Given the complexity of reaching agreement in a number of cases and the consequent difficulties in converting provisionally recorded frequency assignments into definitive recorded assignments, the existing procedure of recording on the basis of four months of interference-free operation should be maintained.

NOC RCC/12A19A7/4

4.1.18*bis* When requesting the application of § 4.1.18, the notifying administration shall undertake to meet the requirements of § 4.1.20 and provide to the administration in respect of which § 4.1.18 is applied, with a copy to the Bureau, a description of the steps by which it undertakes to meet these requirements. Once an assignment is entered in the feeder-link List provisionally under the provisions of § 4.1.18, the calculation of the equivalent protection margin (EPM)[[8]](#footnote-8)11 of an assignment in the Regions 1 and 3 feeder-link List or for which the procedure of Article 4 has been initiated and which was the basis for the disagreement shall not take into account interference produced by the assignment for which the provisions of § 4.1.18 have been applied.     (WRC‑03)

**Reasons:** Given the complexity of reaching agreement in a number of cases and the consequent difficulties in converting provisionally recorded frequency assignments into definitive recorded assignments, the existing procedure of recording on the basis of four months of interference-free operation should be maintained.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \* The expression “frequency assignment to a space station”, wherever it appears in this Appendix, shall be understood to refer to a frequency assignment associated with a given orbital position. See also Annex 7 for the orbital limitations.     (WRC‑2000) [↑](#footnote-ref-1)
2. 1 The Regions 1 and 3 List of additional uses is annexed to the Master International Frequency Register (see Resolution **542 (WRC‑2000)**\*\*).     (WRC‑03)

 \*\* *Note by the Secretariat*: This Resolution was abrogated by WRC‑03.

*Note by the Secretariat*: Reference to an Article with the number in roman is referring to an Article in this Appendix. [↑](#footnote-ref-2)
3. 3 The provisions of Resolution **49 (Rev.WRC‑15)** apply.     (WRC‑15) [↑](#footnote-ref-3)
4. 9 For the definition of EPM, see § 3.4 of Annex 5.     (WRC‑03) [↑](#footnote-ref-4)
5. \* The expression “frequency assignment to a space station”, wherever it appears in this Appendix, shall be understood to refer to a frequency assignment associated with a given orbital position.     (WRC‑03) [↑](#footnote-ref-5)
6. 1 The Regions 1 and 3 feeder-link List of additional uses is annexed to the Master International Frequency Register (see Resolution **542 (WRC‑2000**)\*\*).     (WRC‑03)

 \*\* *Note by the Secretariat*: This Resolution was abrogated by WRC‑03. [↑](#footnote-ref-6)
7. 2 This use of the band 14.5-14.8 GHz is reserved for countries outside Europe.

*Note by the Secretariat*: Reference to an Article with the number in roman is referring to an Article in this Appendix. [↑](#footnote-ref-7)
8. 11 For the definition of the EPM, see § 1.7 of Annex 3.     (WRC‑03) [↑](#footnote-ref-8)