|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Document 30-E** |
|  | **30 September 2019** |
|  | **Original: English** |
|  |
| Mongolia |
| Proposals for the work of the conference |
|  |
| Agenda item 8 |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC-07)**;

Introduction

In accordance with Resolution **26 (Rev.WRC-07)**, the Administration of Mongolia has examined the footnotes to the Table of Frequency Allocations and proposes that the country name of Mongolia be deleted in footnotes No. **5.67**, No. **5.277**, No. **5.455**, No. **5.473**, and No. **5.478**.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD MNG/30/1

5.67 *Additional allocation:*in Kyrgyzstan and Turkmenistan, the band 130-148.5 kHz is also allocated to the radionavigation service on a secondary basis. Within and between these countries this service shall have an equal right to operate.     (WRC‑19)

**Reasons:** There is no radionavigation service usage in the band 130-148.5 kHz in Mongolia. Therefore, the name of Mongolia is no longer required in this footnote.

MOD MNG/30/2

5.277 *Additional allocation:* in Angola, Armenia, Azerbaijan, Belarus, Cameroon, Congo (Rep. of the), Djibouti, the Russian Federation, Georgia, Hungary, Israel, Kazakhstan, Mali, Uzbekistan, Poland, the Dem. Rep. of the Congo, Kyrgyzstan, Slovakia, Romania, Rwanda, Tajikistan, Chad, Turkmenistan and Ukraine, the band 430-440 MHz is also allocated to the fixed service on a primary basis.    (WRC‑19)

**Reasons:** There is no fixed service usage in the band 430-440 MHz in Mongolia. Therefore, to delete the name of Mongolia from this footnote.

MOD MNG/30/3

5.455 *Additional allocation:*in Armenia, Azerbaijan, Belarus, Cuba, the Russian Federation, Georgia, Hungary, Kazakhstan, Moldova, Uzbekistan, Kyrgyzstan, Tajikistan, Turkmenistan and Ukraine, the band 5 670‑5 850 MHz is also allocated to the fixed service on a primary basis.     (WRC-19)

**Reasons:** There is no fixed service usage in the band 5 670-5 850 MHz in Mongolia. Therefore, the name of Mongolia is no longer required in this footnote.

MOD MNG/30/4

5.473 *Additional allocation:*in Armenia, Austria, Azerbaijan, Belarus, Cuba, the Russian Federation, Georgia, Hungary, Uzbekistan, Poland, Kyrgyzstan, Romania, Tajikistan, Turkmenistan and Ukraine, the bands 8 850‑9 000 MHz and 9 200-9 300 MHz are also allocated to the radionavigation service on a primary basis.     (WRC-19)

**Reasons:** There is no radionavigation service usage in the bands 8 850-9 000 MHz and 9 200-9 300 MHz in Mongolia. Therefore, the name of Mongolia is no longer required in this footnote.

MOD MNG/30/5

5.478 *Additional allocation:*in Azerbaijan, Kyrgyzstan, Romania, Turkmenistan and Ukraine, the band 9 800-10 000 MHz is also allocated to the radionavigation service on a primary basis.     (WRC-19)

**Reasons:** There is no radionavigation service usage in the band 9 800-10 000 MHz in Mongolia. Therefore, the name of Mongolia is no longer required in this footnote.