|  |  |  |  |
| --- | --- | --- | --- |
| A close up of a sign  Description automatically generated | **World Radiocommunication Conference (WRC-23) Dubai, 20 November - 15 December 2023** | |  |
|  | |  | |
|  | |  | |
| PLENARY MEETING | | **Document 131-E** | |
|  | | **27 October 2023** | |
|  | | **Original: Russian** | |
|  | | | |
| Belarus (Republic of) | | | |
| proposals for the work of the conference | | | |
|  | | | |
| Agenda item 8 | | | |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC‑19)**;

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

MOD BLR/131/1

5.201 *Additional allocation:*in Armenia, Azerbaijan, Bulgaria, Estonia, the Russian Federation, Georgia, Hungary, Iran (Islamic Republic of), Iraq (Republic of), Japan, Kazakhstan, Mali, Mongolia, Mozambique, Uzbekistan, Papua New Guinea, Poland, Kyrgyzstan, Romania, Senegal, Tajikistan, Turkmenistan and Ukraine, the frequency band 132-136 MHz is also allocated to the aeronautical mobile (OR) service on a primary basis. In assigning frequencies to stations of the aeronautical mobile (OR) service, the administration shall take account of the frequencies assigned to stations in the aeronautical mobile (R) service.     (WRC‑23)

**Reasons:** There is no longer any need to refer to Belarus in this footnote.

MOD BLR/131/2

5.202 *Additional allocation:* in Saudi Arabia, Armenia, Azerbaijan, Bahrain, Bulgaria, the United Arab Emirates, the Russian Federation, Georgia, Iran (Islamic Republic of), Jordan, Mali, Oman, Uzbekistan, Poland, the Syrian Arab Republic, Kyrgyzstan, Romania, Senegal, Tajikistan, Turkmenistan and Ukraine, the frequency band 136-137 MHz is also allocated to the aeronautical mobile (OR) service on a primary basis. In assigning frequencies to stations of the aeronautical mobile (OR) service, the administration shall take account of the frequencies assigned to stations in the aeronautical mobile (R) service.     (WRC‑23)

**Reasons:** There is no longer any need to refer to Belarus in this footnote.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_