|  |  |  |
| --- | --- | --- |
| A close up of a sign  Description automatically generated | **World Radiocommunication Conference (WRC-23)Dubai, 20 November - 15 December 2023** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Document 172-E** |
|  | **30 October 2023** |
|  | **Original: Russian** |
|  |
| Uzbekistan (Republic of) |
| PROPOSALS FOR THE WORK OF THE CONFERENCE |
|  |
| Agenda item 9.2 |

9 to consider and approve the Report of the Director of the Radiocommunication Bureau, in accordance with Article 7 of the ITU Convention;

9.2 on any difficulties or inconsistencies encountered in the application of the Radio Regulations;[[1]](#footnote-1)1

Introduction

In examining the version of the Radio Regulations published in 2020, the Administration of the Republic of Uzbekistan noted a number of inaccuracies, difficulties and mistakes in the English and Russian versions of the texts, among others.

The proposals that follow provide detailed information about proposed editorial changes to Article **5** of the 2020 version of the Radio Regulations to be considered at the Conference under WRC‑23 agenda item 9.2.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD UZB/172/1

40-47.5 GHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| ... |
| 42.5-43.5 FIXED FIXED-SATELLITE (Earth-to-space) 5.552 MOBILE except aeronautical mobile 5.550B RADIO ASTRONOMY 5.149 5.547 5.551H 5.551I |
| ... |

**Reasons:** Information added to fully reflect the conditions in the footnotes to the Table of Frequency Allocations. In this connection it is proposed to complete the text of the Table for the frequency band 42.5-43.5 GHz with footnotes **5.551Н** and **5.551I**, which give the conditions for use by the FSS and BSS with respect to the radio astronomy service in the same band. Concerns all language versions.

MOD UZB/172/2

1 660-1 710 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| ... | ... |
| 1 690-1 700METEOROLOGICAL AIDSMETEOROLOGICAL-SATELLITE (space-to-Earth)FixedMobile except aeronautical mobile | 1 690-1 700 METEOROLOGICAL AIDS METEOROLOGICAL-SATELLITE (space-to-Earth) |
| 5.289 5.341 5.382 |  5.289 5.341 5.381 5.382 |
| ... |  ... |

**Reasons:** In the Radio Regulations, the section of the Table for the frequency band 1 690-1 700 MHz for Regions 2 and 3 is missing a reference to footnote **5.382**, which mentions a *different category of service* for one country in Region 3.

Taking into account RR No. **5.33**, it is proposed to complete the section of the Table for allocations in the frequency band 1 690-1 700 MHz in Regions 2 and 3 with footnote **5.382**. Concerns all language versions.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. 1 This agenda item is strictly limited to the Report of the Director on any difficulties or inconsistencies encountered in the application of the Radio Regulations and the comments from administrations. [↑](#footnote-ref-1)