Draft new Recommendation ITU-T H.225.0 Amendment 1

Call signalling protocols and media stream packetization for packet-based multimedia communication systems:  
Use of FACILITY message to enable call transfer

AAP Summary

This Amendment to H.225.0 formalizes the widely implemented call transfer mechanism in H.323 that relies upon the FACILITY message with a reason of “callForwarded”.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_