**Sipme (country code +883 (5130))**

Communication of 14.I.2014:

*SIPME Limited*, Kiryat Motzkin, recalls that the International Telecommunication Union (ITU) assigned the E.164 shared country code and identification code +883 5130 to Sipme Ltd on 16 September 2013 and it is being introduced on 1ST January 2014. Provisions must therefore be made in all countries with immediate effect, for callers to be able to dial the country code +883 5130 followed by the Subscriber Number (SN).

The initial +883 5130 dialling plan will consist of +883 5130 followed by eight (8) digits, (i.e +883 5130 XXXX XXXX).

|  |  |  |  |
| --- | --- | --- | --- |
| *NDC (National Destination Code) or leading digits of N(S)N (National (Significant) Number)* | *N(S) number length* | *Usage of E.164 Number* | *Additional Information* |
| *Maximum length* | *Minimum length* |
| (883) - 5130 | 8 | 8 | Non-geographic number for telephony services (VOIP) | Assigned to Sipme Ltd,Reference: COM 2-2367/MJ |

\* International dialling format: + 883 5130 XXXX XXXX

Sipme has a Transit-Carrier Agreement with Bezeq International (Israel). Traffic to the E.164 shared country code and identification code +883 5130 received from any of your customers needs to be sent to Bezeq International for termination (Point Code 4-004-0 & 4-004-1).

Contacts for any subject

 CTO: Mr. Tamir Avigdor, Tel: +972 54 2040300, E-mail: ta@sipme.me
CEO: Mr. Yulian Oifa, Tel: +972 52 5953366, E-mail: yulian\_o@sipme.me