|  |  |  |  |
| --- | --- | --- | --- |
| AUS - Australia | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Australian Communications and Media Authority | International Radiocommunications Section P.O. Box 78 Belconnen A.C.T. 2616 | TF : +61 2 62195555 FAX : +61 2 62195353 EMAIL : info@acma.gov.au EMAIL : irs@acma.gov.au |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Quoin Ridge (Tasmania)** | ACMA Quoin Ridge P.O. Box 13112 Law Courts Melbourne Victoria 8010 Australia | TF : +61 3 99636702 FAX : +61 3 62680246 EMAIL : quoin.ridge@acma.gov.au | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 42°45'00''S 147°20'00''E | Frequency measurements | 10 kHz - 2 GHz | HX |  |
| 42°45'00''S 147°20'00''E | Field strength or power flux-density measurements | 10 kHz - 2 GHz | HX |  |
| 42°45'00''S 147°20'00''E | Direction-finding measurements | 100 kHz - 40 MHz | H24 | Superresolution DF with better than ± 0.5 degrees dependent on the signal to noise ratio of the wanted signal. |
| 42°45'00''S 147°20'00''E | Bandwidth measurements | 10 kHz - 2 GHz | HX |  |
| 42°45'00''S 147°20'00''E | Automatic spectrum occupancy surveys | 10 kHz - 2 GHz | H24 |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_