|  |  |  |  |
| --- | --- | --- | --- |
| AUT - Austria | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Federal Ministry of Finance Directorate-General VI/3 Centralizing Office for Monitoring | Radetzkystrasse 2 1030 Wien | PHONE: +43 1 51433 506424 EMAIL: ernst.cerny@bmf.gv.at EMAIL: post.vi-3@bmf.gv.at |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Wien (IMS)** | Fernmeldebüro, Telecommunications Authority Republic Austria 17 Krapfenwaldgasse 1190 Wien Austria | PHONE: +43 1 71100 654488 EMAIL: funkmonitoring@fb.gv.at | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 48°19'41"N 016°28'42"E | Direction-finding measurements | (100) 500 kHz - 30 MHz | HX | Correlative interferometer. |
| 48°15'45"N 016°20'08"E | Direction-finding measurements | 30 MHz - 3 GHz | H24 | If necessary, direction-finding measurements are carried out by mobile monitoring stations (van).  Correlation. |
| 48°15'45"N 016°20'08"E | Frequency measurements | 9 kHz - 90 GHz | H24 |  |
| 48°15'45"N 016°20'08"E | Field strength or power flux-density measurements | 9 kHz - 90 GHz | H24 | If necessary, measurements are carried out by mobile monitoring stations (van). |
| 48°15'45"N 016°20'08"E | Bandwidth measurements | 9 kHz - 90 GHz | H24 | If necessary, measurements are carried out by mobile monitoring stations (van). |
| 48°15'45"N 016°20'08"E | Automatic spectrum occupancy surveys | 9 kHz - 90 GHz | H24 |  |
| 46°38'07"N 014°29'43"E | Frequency measurements | 9 kHz - 30 MHz | HX |  |
| 46°38'07"N 014°29'43"E | Field strength or power flux-density measurements | 9 kHz - 30 MHz | HK |  |
| 46°38'07"N 014°29'43"E | Direction-finding measurements | (100) 300 kHz - 30 MHz | HX | Correlative interferometer. |
| 43°38'08"N 014°29'43"E | Automatic spectrum occupancy surveys | 9 kHz - 30 MHz | HX |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_