|  |  |  |  |
| --- | --- | --- | --- |
| CLM - Colombia | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Sección Control y Registro  Técnico de Frecuencias  Ministerio de Comunicaciones | Edificio Murillo Toro Bogotá | TF : +57 1 2832735 TF : +57 1 2866911 Ext. 392 TF : +57 1 2432378 |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **El Caribe (Barranquilla-Atlántico)** | Apdo. Aéreo 4376  Barranquilla Colombia | TF : +57 5 513033 TF : +57 5 513122 FAX : +57 5 513033 FAX : +57 5 513122 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 10°59'11''N 074°46'43''W | Frequency measurements | 10 kHz - 1 GHz | 0600-2000 |  |
| 10°59'11''N 074°46'43''W | Field strength or power flux-density measurements | 150 kHz - 32 MHz | 0600-2000 |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **El Cerrito (Funza-Cundinamarca)** | Ed. Murillo Toro Cra. 7 C11. 12A Bogotá D.C. Colombia | TF : +57 1 2670180 TF : +57 1 2866911 TF : +57 1 2671663 TF : +57 1 2670182 TF : +57 1 2670181 FAX : +57 1 2671663 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 04°42'54''N 074°10'46''W | Frequency measurements | 10 kHz - 30 MHz |  | 1100-0100 h. |
| 04°42'54''N 074°10'46''W | Frequency measurements | 20 MHz - 1 GHz |  | 1100-0100 h. |
| 04°42'54''N 074°10'46''W | Field strength or power flux-density measurements | 10 kHz - 32 MHz |  | 1100-0100 h. |
| 04°42'54''N 074°10'46''W | Field strength or power flux-density measurements | 20 MHz - 1 GHz |  | 1100-0100 h. |
| 04°42'54''N 074°10'46''W | Direction-finding measurements | 5 kHz - 30 MHz |  | Doppler antenna.  Fixed direction-finding station.  1200-2400 h. |
| 04°42'54''N 074°10'46''W | Direction-finding measurements | 20 MHz - 1000 MHz |  | U-Adcock.  Mobile direction-finding station.  1200-2400 h. |
| 04°42'54''N 074°10'46''W | Bandwidth measurements | 50 Hz - 2 GHz |  | 1100-0100 h. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **El Mirador (Cúcuta-N. Santander)** | Apdo. Aéreo 777 Cúcuta Colombia | TF : +57 70 760809 TF : +57 70 760702 FAX : +57 70 741000 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 07°45'00''N 072°30'00''W | Frequency measurements | 10 kHz - 1 GHz | 0600-2000 |  |
| 07°45'00''N 072°30'00''W | Field strength or power flux-density measurements | 10 kHz - 1 GHz | 0600-2000 |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **La Sultana (Candelaria-Valle)** | Apdo. Aéreo 293 Cali Colombia | TF : +57 2 839219 TF : +57 2 839220 FAX : +57 2 8839220 FAX : +57 2 8834008 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 03°22'46''N 076°25'01''W | Frequency measurements | 9 kHz - 30 MHz | 0600-2000 |  |
| 03°22'46''N 076°25'01''W | Frequency measurements | 20 MHz - 1000 MHz | 0600-2000 |  |
| 03°22'46''N 076°25'01''W | Field strength or power flux-density measurements | 150 kHz - 32 MHz | 0600-2000 |  |
| 03°22'46''N 076°25'01''W | Field strength or power flux-density measurements | 20 MHz - 1000 MHz | 0600-2000 |  |
| 03°22'46''N 076°25'01''W | Bandwidth measurements | 10 kHz - 1000 MHz |  | 1200-2400 h. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Llano Grande (Rionegro-Antioquia)** | Apdo. Aéreo 2882 Medellín Apartado Aéreo 152 Rionegro-Antioquia Colombia | TF : +57 4 5370354 TF : +57 4 5370334 FAX : +57 4 5371103 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 06°12'00''N 075°23'00''W | Frequency measurements | 10 kHz - 1000 MHz | 1100-0100 |  |
| 06°12'00''N 075°23'00''W | Field strength or power flux-density measurements | 150 kHz - 32 MHz | 1100-0100 |  |
| 06°12'00''N 075°23'00''W | Bandwidth measurements | 20 MHz - 1000 MHz | 1100-0100 |  |
| 06°12'00''N 075°23'00''W | Automatic spectrum occupancy surveys |  | 1100-0100 | 99 channels between 20 MHz and 1000 MHz. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Los Comuneros (Bucaramanga-Santander)** | Apdo. Aéreo 3701  Bucaramanga Colombia | TF : +57 7 361659 FAX : +57 7 361653 FAX : +57 7 361639 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 07°06'00''N 073°08'00''W | Frequency measurements | 9 kHz - 1 GHz |  | 1100-0100 h. |
| 07°06'00''N 073°08'00''W | Field strength or power flux-density measurements | 150 kHz - 32 MHz |  | 1100-0100 h. |
| 07°06'00''N 073°08'00''W | Bandwidth measurements | 9 kHz - 1 GHz |  | 1100-0100 h. |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_