|  |  |  |  |
| --- | --- | --- | --- |
| F - France | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Agence Nationale des Fréquences (ANFR)  Direction Technique du Contrôle du Spectre | 112, rue Édouard Vaillant 94815 Villejuif Cedex France | TF : +33 1 49583146 FAX : +33 1 49583129 EMAIL : bcn@anfr.fr URL : www.anfr.fr |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Favières (IMS)** | Centre de Contrôle des Fréquences CSTEI Favières BP 10019 28170 Favières France | TF : +33 2 37385415 TF : +33 2 37385392 FAX : +33 2 37385418 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 48°32'27''N 001°14'03''E | Frequency measurements | 2 MHz - 30 MHz | H24 |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Rambouillet (IMS)** | Centre de Contrôle International de Rambouillet Avenue de Cerqueuse 78660 Prunay en Yvelines France | TF : +33 1 34941700 FAX : +33 1 34941720 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 48°32'58''N 001°47'38''E | Frequency measurements | 10 kHz - 30 MHz | H24 | Measurements also carried out by mobile stations (0830-1730). |
| 48°32'58''N 001°47'38''E | Frequency measurements | 20 MHz - 3 GHz | H24 | Measurements also carried out by mobile stations (0830-1730). |
| 48°32'58''N 001°47'38''E | Frequency measurements | 1 GHz - 40 GHz | 0830-1730 | Measurements also carried out by mobile stations (0830-1730). |
| 48°32'58''N 001°47'38''E | Field strength or power flux-density measurements | 10 kHz - 30 MHz | H24 | Measurements also carried out by mobile stations (0830-1730). |
| 48°32'58''N 001°47'38''E | Field strength or power flux-density measurements | 20 MHz - 3 GHz | 0830-1730 | Measurements also carried out by mobile stations (0830-1730). |
| 48°32'58''N 001°47'38''E | Field strength or power flux-density measurements | 1 GHz - 40 GHz | 0830-1730 | Measurements also carried out by mobile stations (0830-1730). |
| 48°32'58''N 001°47'38''E | Direction-finding measurements | 300 kHz - 30 MHz | H24 | Localization by means of a direction-finding network equipped with Adcock antennas and a single localization station situated at the Rambouillet International Monitoring Center. |
| 48°32'58''N 001°47'38''E | Direction-finding measurements | 20 MHz - 3 GHz | H24 | Interferometry. |
| 48°32'58''N 001°47'38''E | Bandwidth measurements | 10 kHz - 3 GHz | H24 |  |
| 48°32'58''N 001°47'38''E | Bandwidth measurements | 1 GHz - 40 GHz | 0830-1730 |  |
| 48°32'58''N 001°47'38''E | Automatic spectrum occupancy surveys | 10 kHz - 30 MHz | H24 |  |
| 48°32'58''N 001°47'38''E | Automatic spectrum occupancy surveys | 20 kHz - 3 GHz | H24 |  |
| 48°32'58''N 001°47'38''E | Automatic spectrum occupancy surveys | 1 GHz - 40 GHz | 0830-1730 |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_