|  |
| --- |
| MTN - Mauritania |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Autorité de Régulation Direction des TélécommunicationsService de gestion et contrôle du spectre de fréquences | B.P. 4908Nouakchott | TF : +222 45291270FAX : +222 45291279EMAIL : m.ahmed@are.mrEMAIL : m.bourweiss@are.mr |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Centre Boghé**  | BP 4908NouakchottMauritanie   | TF : +222 43381526FAX : +222 45291279EMAIL : wedoud1526@yahoo.fr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 16°35'23''N014°16'24''W | Frequency measurements   | 20 MHz - 3 GHz   | H24   |   |
| 16°35'23''N014°16'24''W | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | H24   |   |
| 16°35'23''N014°16'24''W | Direction-finding measurements   | 20 MHz - 3 GHz   | H24   |   |
| 16°35'23''N014°16'24''W | Bandwidth measurements   | 20 MHz - 3 GHz   | H24   |   |
| 16°35'23''N014°16'24''W | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Centre Nbeiket Lahwache**  | BP 4908NouakchottMauritanie   | TF : +222 43333001FAX : +222 45291279EMAIL : m.bourweiss@are.mrEMAIL : bramy@yahoo.fr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 16°50'24''N005°57'12''W | Frequency measurements   | 9 kHz - 3 GHz   | H24   |   |
| 16°50'24''N005°57'12''W | Field strength or power flux-density measurements   | 9 kHz - 3 GHz   | H24   |   |
| 16°50'24''N005°57'12''W | Direction-finding measurements   | 9 kHz - 3 GHz   | H24   |   |
| 16°50'24''N005°57'12''W | Bandwidth measurements   | 9 kHz - 3 GHz   | H24   |   |
| 16°50'24''N005°57'12''W | Automatic spectrum occupancy surveys   | 9 kHz - 3 GHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Centre Nouadhibou**  | B.P. 4908NouakchottMauritanie   | TF : +222 46491649FAX : +222 45291279EMAIL : ayah26@gmail.com   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 20°57'51''N017°02'29''W | Frequency measurements   | 9 kHz - 3 GHz   | H24   |   |
| 20°57'51''N017°02'29''W | Field strength or power flux-density measurements   | 9 kHz - 3 GHz   | H24   |   |
| 20°57'51''N017°02'29''W | Direction-finding measurements   | 9 kHz - 3 GHz   | H24   |   |
| 20°57'51''N017°02'29''W | Bandwidth measurements   | 9 kHz - 3 GHz   | H24   |   |
| 20°57'51''N017°02'29''W | Automatic spectrum occupancy surveys   | 9 kHz - 3 GHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Centre Riadh**  | BP 4908NouakchottMauritanie   | TF : +222 46412919FAX : +222 45291279EMAIL : ahvall.md@are.mrEMAIL : m.bourweiss@are.mr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 17°59'26''N015°57'13''W | Frequency measurements   | 9 kHz - 3 GHz   | H24   |   |
| 17°59'26''N015°57'13''W | Field strength or power flux-density measurements   | 9 kHz - 3 GHz   | H24   |   |
| 17°59'26''N015°57'13''W | Direction-finding measurements   | 9 kHz - 3 GHz   | H24   |   |
| 17°59'26''N015°57'13''W | Bandwidth measurements   | 9 kHz - 3 GHz   | H24   |   |
| 17°59'26''N015°57'13''W | Automatic spectrum occupancy surveys   | 9 kHz - 3 GHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Centre Selibaby**  | BP 4908NouakchottMauritanie   | TF : +222 46471548 FAX : +222 45291279EMAIL : m.bourweiss@are.mrEMAIL : souheib@live.fr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 15°10'29''N012°11'20''W | Frequency measurements   | 20 MHz - 3 GHz   | H24   |   |
| 15°10'29''N012°11'20''W | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   | H24   |   |
| 15°10'29''N012°11'20''W | Direction-finding measurements   | 20 MHz - 3 GHz   | H24   |   |
| 15°10'29''N012°11'20''W | Bandwidth measurements   | 20 MHz - 3 GHz   | H24   |   |
| 15°10'29''N012°11'20''W | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Centre Zouérate**  | BP 4908NouakchottMauritanie   | TF : +222 43505016FAX : +222 45291279EMAIL : boukreiss@hotmail.fr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 22°45'00''N012°27'29''W | Frequency measurements   | 9 kHz - 3 GHz   | H24   |   |
| 22°45'00''N012°27'29''W | Field strength or power flux-density measurements   | 9 kHz - 3 GHz   | H24   |   |
| 22°45'00''N012°27'29''W | Direction-finding measurements   | 9 kHz - 3 GHz   | H24   |   |
| 22°45'00''N012°27'29''W | Bandwidth measurements   | 9 kHz - 3 GHz   | H24   |   |
| 22°45'00''N012°27'29''W | Automatic spectrum occupancy surveys   | 9 kHz - 3 GHz   | H24   |   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Mobile I**  | BP 4908NouakchottMauritanie   | TF : +222 43505014FAX : +222 45291279EMAIL : m.bourweiss@are.mrEMAIL : mm.cheikh@are.mr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
|   | Frequency measurements   | 9 kHz - 8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Field strength or power flux-density measurements   | 9 kHz - 8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Direction-finding measurements   | 9 kHz - 8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Bandwidth measurements   | 9 kHz - 8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Automatic spectrum occupancy surveys   | 9 kHz - 8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Mobile II**  | BP 4908NouakchottMauritanie   | TF : +222 43505014FAX : +222 45291279EMAIL : mm.cheikh@are.mrEMAIL : m.bourweiss@are.mr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
|   | Frequency measurements   | 9 kHz -8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Field strength or power flux-density measurements   | 9 kHz -8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Direction-finding measurements   | 9 kHz -8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Bandwidth measurements   | 9 kHz -8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |
|   | Automatic spectrum occupancy surveys   | 9 kHz -8 GHz   | H24   | Our mobile stations are compatible with fixed stations.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Nouakchott**  | B.P. 4908NouakchottMauritanie   | TF : +222 521 0643FAX : +222 529 1279EMAIL : vtabou@are.mrEMAIL : baoumar6486304@yahoo.fr   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 17°59'25''N015°57'12''W | Frequency measurements   | 9 kHz - 3 GHz   | H24   | Network composed of a spectrum management computerized system and 2 fixed stations and 2 mobile stations.   |
| 17°59'25''N015°57'12''W | Field strength or power flux-density measurements   | 9 kHz - 3 GHz   | H24   |   |
| 17°59'25''N015°57'12''W | Direction-finding measurements   | 9 kHz - 3 GHz   | H24   | Two antennas: an UHF antenna of 9 elements and 1 element of reference, and a VHF antenna of 5 elements.   |
| 17°59'25''N015°57'12''W | Bandwidth measurements   | 9 kHz - 3 GHz   | H24   |   |
| 17°59'25''N015°57'12''W | Automatic spectrum occupancy surveys   | 9 kHz - 3 GHz   | H24   |   |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_