|  |
| --- |
| SVN - Slovenia |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| AKOSAgency for communication networks and services of the Republic of Slovenia | Stegne 7 P.O. Box 4181001 Ljubljana | TF : +386 1 5836300FAX : +386 1 5111101EMAIL : info.box@akos-rs.si |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Brežice**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°51'46''N015°38'38''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°51'46''N015°38'38''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°51'46''N015°38'38''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 45°51'46''N015°38'38''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°51'46''N015°38'38''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Celje**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°17'13''N015°13'00''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°17'13''N015°13'00''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°17'13''N015°13'00''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°17'13''N015°13'00''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°17'13''N015°13'00''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Dravograd**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°37'09''N015°02'12''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°37'09''N015°02'12''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°37'09''N015°02'12''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°37'09''N015°02'12''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°37'09''N015°02'12''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Jeruzalem**  | P.O. Box 159240 LjutomerSlovenia   | TF : +386 2 7400221FAX : +386 2 7400220EMAIL : rnpj@siol.net   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°28'45''N016°11'24''E | Frequency measurements   | 9 kHz - 30 GHz   | 0730-1530   | Manned monitoring station.Working days.   |
| 46°28'45''N016°11'24''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.   |
| 46°28'45''N016°11'24''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°28'45''N016°11'24''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.   |
| 46°28'45''N016°11'24''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Koper**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°30'08''N013°44'23''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°30'08''N013°44'23''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°30'08''N013°44'23''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 45°30'08''N013°44'23''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°30'08''N013°44'23''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Ljubljana**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°02'46''N014°29'30''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°02'46''N014°29'30''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°02'46''N014°29'30''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°02'46''N014°29'30''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°02'46''N014°29'30''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Maribor**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°35'58''N015°31'47''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730 - 1530   | Remotely controlled monitoring station.Working days.   |
| 46°35'58''N015°31'47''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730 - 1530   | Remotely controlled monitoring station.Working days.   |
| 46°35'58''N015°31'47''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730 - 1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°35'58''N015°31'47''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730 - 1530   | Remotely controlled monitoring station.Working days.   |
| 46°35'58''N015°31'47''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730 - 1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Nova Gorica**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°59'28''N013°37'54''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°59'28''N013°37'54''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°59'28''N013°37'54''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 45°59'28''N013°37'54''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°59'28''N013°37'54''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Novo mesto**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°48'06''N015°10'37''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°48'06''N015°10'37''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°48'06''N015°10'37''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 45°48'06''N015°10'37''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 45°48'06''N015°10'37''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Rašica**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°08'23''N014°30'44''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°08'23''N014°30'44''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°08'23''N014°30'44''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°08'23''N014°30'44''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°08'23''N014°30'44''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Sevnica**  | Slovenia   |   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°02'09''N015°09'26''E | Frequency measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°02'09''N015°09'26''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°02'09''N015°09'26''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°02'09''N015°09'26''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.   |
| 46°02'09''N015°09'26''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Remotely controlled monitoring station.Working days.Selected subrange in the frequency band.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Stegne**  | Stegne 7P.O. Box 4181001 LjubljanaSlovenia   | TF : +386 1 5836300FAX : +386 1 5111101   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°05'02''N014°29'10''E | Frequency measurements   | 9 kHz - 40 GHz   | 0730-1530   | Manned monitoring station.Working days.   |
| 46°05'02''N014°29'10''E | Field strength or power flux-density measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.   |
| 46°05'02''N014°29'10''E | Direction-finding measurements   | 50 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.Log-periodic antenna (0° – 359°) vertical/horizontal.   |
| 46°05'02''N014°29'10''E | Bandwidth measurements   | 25 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.   |
| 46°05'02''N014°29'10''E | Automatic spectrum occupancy surveys   | 25 MHz - 2.7 GHz   | 0730-1530   | Manned monitoring station.Working days.Selected subrange in the frequency band.   |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_