|  |  |  |  |
| --- | --- | --- | --- |
| SVN - Slovenia | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| AKOS Agency for communication networks and services of the Republic of Slovenia | Stegne 7  P.O. Box 418 1001 Ljubljana | TF : +386 1 5836300 FAX : +386 1 5111101 EMAIL : info.box@akos-rs.si |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Brežice** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°51'46''N 015°38'38''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°51'46''N 015°38'38''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°51'46''N 015°38'38''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 45°51'46''N 015°38'38''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°51'46''N 015°38'38''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Celje** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°17'13''N 015°13'00''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°17'13''N 015°13'00''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°17'13''N 015°13'00''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°17'13''N 015°13'00''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°17'13''N 015°13'00''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Dravograd** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°37'09''N 015°02'12''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°37'09''N 015°02'12''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°37'09''N 015°02'12''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°37'09''N 015°02'12''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°37'09''N 015°02'12''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Jeruzalem** | P.O. Box 15 9240 Ljutomer Slovenia | TF : +386 2 7400221 FAX : +386 2 7400220 EMAIL : rnpj@siol.net | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°28'45''N 016°11'24''E | Frequency measurements | 9 kHz - 30 GHz | 0730-1530 | Manned monitoring station.  Working days. |
| 46°28'45''N 016°11'24''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days. |
| 46°28'45''N 016°11'24''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°28'45''N 016°11'24''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days. |
| 46°28'45''N 016°11'24''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Koper** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°30'08''N 013°44'23''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°30'08''N 013°44'23''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°30'08''N 013°44'23''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 45°30'08''N 013°44'23''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°30'08''N 013°44'23''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Ljubljana** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°02'46''N 014°29'30''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°02'46''N 014°29'30''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°02'46''N 014°29'30''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°02'46''N 014°29'30''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°02'46''N 014°29'30''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Maribor** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°35'58''N 015°31'47''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730 - 1530 | Remotely controlled monitoring station.  Working days. |
| 46°35'58''N 015°31'47''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730 - 1530 | Remotely controlled monitoring station.  Working days. |
| 46°35'58''N 015°31'47''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730 - 1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°35'58''N 015°31'47''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730 - 1530 | Remotely controlled monitoring station.  Working days. |
| 46°35'58''N 015°31'47''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730 - 1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Nova Gorica** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°59'28''N 013°37'54''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°59'28''N 013°37'54''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°59'28''N 013°37'54''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 45°59'28''N 013°37'54''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°59'28''N 013°37'54''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Novo mesto** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 45°48'06''N 015°10'37''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°48'06''N 015°10'37''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°48'06''N 015°10'37''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 45°48'06''N 015°10'37''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 45°48'06''N 015°10'37''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Rašica** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°08'23''N 014°30'44''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°08'23''N 014°30'44''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°08'23''N 014°30'44''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°08'23''N 014°30'44''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°08'23''N 014°30'44''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Sevnica** | Slovenia |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°02'09''N 015°09'26''E | Frequency measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°02'09''N 015°09'26''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°02'09''N 015°09'26''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°02'09''N 015°09'26''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days. |
| 46°02'09''N 015°09'26''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Remotely controlled monitoring station.  Working days.  Selected subrange in the frequency band. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Stegne** | Stegne 7 P.O. Box 418 1001 Ljubljana Slovenia | TF : +386 1 5836300 FAX : +386 1 5111101 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 46°05'02''N 014°29'10''E | Frequency measurements | 9 kHz - 40 GHz | 0730-1530 | Manned monitoring station.  Working days. |
| 46°05'02''N 014°29'10''E | Field strength or power flux-density measurements | 25 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days. |
| 46°05'02''N 014°29'10''E | Direction-finding measurements | 50 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days.  Log-periodic antenna (0° – 359°) vertical/horizontal. |
| 46°05'02''N 014°29'10''E | Bandwidth measurements | 25 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days. |
| 46°05'02''N 014°29'10''E | Automatic spectrum occupancy surveys | 25 MHz - 2.7 GHz | 0730-1530 | Manned monitoring station.  Working days.  Selected subrange in the frequency band. |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_