|  |
| --- |
| VTN - Viet Nam |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| Authority of Radio Frequency Management | 115, Tran Duy Hung streetCau Giay districtHa Noi City | TF : +84 345564926FAX : +84 345564930EMAIL : KiemsoatTS@rfd.gov.vn |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Can Tho**  | 386A, Cach Mang Thang Tam streetCan Tho CityViet Nam   | TF : +84 7103832761FAX : +84 7103887087EMAIL : dks.tt4@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 10°03'53''N105°45'43''E | Frequency measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 10°03'53''N105°45'43''E | Frequency measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 10°03'53''N105°45'43''E | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 10°03'53''N105°45'43''E | Direction-finding measurements   | 0.5 MHz - 30 MHz   |   | H24: on request.Semi-fixed station.Active U-Adcock HF direction-finding antenna (1 MHz to 30 MHz).Active HF ferrite antenna (0.5 MHz to 30 MHz) while moving.   |
| 10°03'53''N105°45'43''E | Direction-finding measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 10°03'53''N105°45'43''E | Bandwidth measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 10°03'53''N105°45'43''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 10°03'53''N105°45'43''E | Automatic spectrum occupancy surveys   | 30 MHz - 3 GHz   |   | H24: on request.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Da Nang**  | Lo C1, Tran Hung Dao streetSon Tra districtDa Nang CityViet Nam   | TF : +84 5113933353FAX : +84 5113933707EMAIL : dks.tt3@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 16°03'11''N108°13'59''E | Frequency measurements   | 9 kHz - 30 MHz   |   | H24: on request.   |
| 16°03'11''N108°13'59''E | Frequency measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 16°03'11''N108°13'59''E | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 16°03'11''N108°13'59''E | Direction-finding measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 16°03'11''N108°13'59''E | Bandwidth measurements   | 9 kHz - 30 MHz   |   | H24: on request.   |
| 16°03'11''N108°13'59''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 16°03'11''N108°13'59''E | Automatic spectrum occupancy surveys   | 30 MHz - 3 GHz   |   | H24: on request.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Ha Noi**  | 115, Tran Duy Hung streetCau Giay districtHanoi CityViet Nam   | TF : +84 345564919FAX : +84 345564913EMAIL : dks.tt1@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 21°00'32''N105°47'53''E | Frequency measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 21°00'32''N105°47'53''E | Frequency measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 21°00'32''N105°47'53''E | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 21°00'32''N105°47'53''E | Direction-finding measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 21°00'32''N105°47'53''E | Bandwidth measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 21°00'32''N105°47'53''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 21°00'32''N105°47'53''E | Automatic spectrum occupancy surveys   | 30 MHz - 3 GHz   |   | H24: on request.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Hai Phong**  | 783, Ton Duc Thang streetHong Bang districtHai Phong CityViet Nam   | TF : +84 313827856FAX : +84 313827420EMAIL : dks.tt5@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 20°51'38''N106°38'59''E | Frequency measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 20°51'38''N106°38'59''E | Frequency measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 20°51'38''N106°38'59''E | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 20°51'38''N106°38'59''E | Direction-finding measurements   | 0.5 MHz - 30 MHz   |   | H24: on request.Semi-fixed station.Active U-Adcock HF direction-finding antenna (1 MHz to 30 MHz).Active HF ferrite antenna (0.5 MHz to 30 MHz) while moving.   |
| 20°51'38''N106°38'59''E | Direction-finding measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 20°51'38''N106°38'59''E | Bandwidth measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 20°51'38''N106°38'59''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 20°51'38''N106°38'59''E | Automatic spectrum occupancy surveys   | 30 MHz - 3 GHz   |   | H24: on request.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Ho Chi Minh**  | Lot 6 Area EAn Phu An Khanh, District 2Ho Chi Minh CityViet Nam   | TF : +84 837404179FAX : +84 837404966EMAIL : dks.tt2@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 10°47'42''N106°44'26''E | Frequency measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 10°47'42''N106°44'26''E | Frequency measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 10°47'42''N106°44'26''E | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 10°47'42''N106°44'26''E | Direction-finding measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 10°47'42''N106°44'26''E | Bandwidth measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 10°47'42''N106°44'26''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 10°47'42''N106°44'26''E | Automatic spectrum occupancy surveys   | 30 MHz - 3 GHz   |   | H24: on request.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Nha Trang**  | Vinh Thanh wardNha Trang CityViet Nam   | TF : +84 583892567FAX : +84 583892020EMAIL : dks.tt7@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 12°15'32''N109°09'23''E | Frequency measurements   | 9 kHz - 30 MHz   |   | H24: on request.   |
| 12°15'32''N109°09'23''E | Frequency measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 12°15'32''N109°09'23''E | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 12°15'32''N109°09'23''E | Direction-finding measurements   | 20 MHz -3 GHz   |   | H24: on request.   |
| 12°15'32''N109°09'23''E | Bandwidth measurements   | 9 kHz - 30 MHz   |   | H24: on request.   |
| 12°15'32''N109°09'23''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 12°15'32''N109°09'23''E | Automatic spectrum occupancy surveys   | 30 MHz -3 GHz   |   | H24: on request.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Viet Tri (IMS)** | Duu Lau wardViet Tri CityViet Nam   | TF : +84 2103840505FAX : +84 2103840504EMAIL : dks.tt8@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 21°20'21''N105°24'24''E | Frequency measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 21°20'21''N105°24'24''E | Frequency measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 21°20'21''N105°24'24''E | Field strength or power flux-density measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 21°20'21''N105°24'24''E | Direction-finding measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 21°20'21''N105°24'24''E | Bandwidth measurements   | 10 kHz - 30 MHz   |   | H24: on request.   |
| 21°20'21''N105°24'24''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 21°20'21''N105°24'24''E | Automatic spectrum occupancy surveys   | 30 MHz - 3 GHz   |   | H24: on request.   |

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Vinh**  | 19, Le Nin streetVinh CityViet Nam   | TF : +84 383849519FAX : +84 383849518EMAIL : dks.tt6@rfd.gov.vn   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 18°41'02''N105°41'32''E | Frequency measurements   | 9 kHz - 30 MHz   |   | H24: on request.   |
| 18°41'02''N105°41'32''E | Frequency measurements   | 30 MHz -3 GHz   |   | H24: on request.   |
| 18°41'02''N105°41'32''E | Field strength or power flux-density measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 18°41'02''N105°41'32''E | Direction-finding measurements   | 20 MHz - 3 GHz   |   | H24: on request.   |
| 18°41'02''N105°41'32''E | Bandwidth measurements   | 30 MHz - 3 GHz   |   | H24: on request.   |
| 18°41'02''N105°41'32''E | Automatic spectrum occupancy surveys   | 20 MHz - 3 GHz   |   | H24: on request.   |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_