Volunteer                                          Vidyo
Description                                        ST-4 + deblocking controls, disable_deblocking_filter_idc=3, disable_inter_layer_deblocking_filter_idc=2
Scalability Type                                   Spatial/Temporal     
Bitstream                                          SVCBST-8 
Bitstream Number                                   1      
Width                                              720    
Height                                             480   
Frame rate                                         30.00  
Number of frames                                   100   
chroma_format_idc                                  1      
bit_depth_luma_minus8                              0      
bit_depth_chroma_minus8                            0      
residual_color_transform_flag                      -      
separate_colour_plane_flag                         -      
profile_idc                                        83     
level_idc                                          40     
constraint_set0_flag                               1      
constraint_set1_flag                               0      
constraint_set2_flag                               0      
constraint_set3_flag                               0      
Number of IDR access units                         1      
Number of slices per picture                       >1      
seq_scaling_matrix_present_flag                    0      
transform_8x8_mode_flag                            0      
pic_scaling_matrix_present_flag                    0      
qpprime_y_zero_transform_bypass_flag               0      
slice_qp_delta == 0                                0      
mb_qp_delta == 0                                   0      
chroma_qp_index_offset                             0      
frame_mbs_only_flag                                1      
mb_adaptive_frame_field_flag                       -      
field_pic_flag                                     -      
deblocking_filter_control_present_flag             1      
disable_deblocking_filter_idc                      3     
slice_alpha_c0_offset_div2                         !=0      
slice_beta_offset_div2                             !=0      
entropy_coding_mode_flag                           1      
I_PCM                                              -      
direct_spatial_mv_pred_flag                        -      
direct_8x8_inference_flag                          1      
weighted_pred_flag                                 0      
weighted_bipred_idc                                0      
num_ref_frames                                     4      
gaps_in_frame_num_value_allowed_flag               1      
ref_pic_list_reordering_flag                       1      
adaptive_ref_pic_marking_mode_flag                 1      
num_slice_groups_minus1                            0      
slice_group_map_type                               -      
pic_order_cnt_type                                 2      
frame_cropping_flag                                1      
VUI                                                -      
HRD                                                -      
SEI                                                1      
priority_id                                        0      
dependency_id                                      1      
quality_id                                         0      
ref_layer_dq_id                                    0      
DependencyIdMax                                    1      
TemporalIdMax                                      3      
DQIdMax                                            16      
DependentDId                                              
Number of EIDR slices                              >1      
extended_spatial_scalability                       0      
SpatialResolutionChangeFlag                        1      
chroma_phase_x_plus1_flag                          1      
chroma_phase_y_plus1                               1      
seq_ref_layer_chroma_phase_x_plus1_flag            -      
seq_ref_layer_chroma_phase_y_plus1                 -      
seq_scaled_ref_layer_left_offset                   -      
seq_scaled_ref_layer_top_offset                    -      
seq_scaled_ref_layer_right_offset                  -      
seq_scaled_ref_layer_bottom_offset                 -      
ref_layer_chroma_phase_x_plus1_flag                       
ref_layer_chroma_phase_y_plus1                            
constrained_intra_resampling_flag                  1      
no_inter_layer_pred_flag                           0      
use_ref_base_pic_flag                              0      
store_ref_base_pic_flag                            0      
output_flag                                        1      
discardable_flag                                   0      
slice_header_restriction_flag                      0      
scan_idx_start                                     0      
scan_idx_end                                       15     
seq_tcoeff_level_prediction_flag                   0      
adaptive_tcoeff_level_prediction_flag              -      
slice_skip_flag                                    0      
num_mbs_in_slice_minus1                            -      
adaptive_base_mode_flag                            1      
default_base_mode_flag                             -      
adaptive_motion_prediction_flag                    0      
default_motion_prediction_flag                     1      
adaptive_residual_prediction_flag                  1      
default_residual_prediction_flag                   -      
base_pred_weight_table_flag                        -      
inter_layer_deblocking_filter_control_present_flag 1      
disable_inter_layer_deblocking_filter_idc          2      
inter_layer_slice_alpha_c0_offset_div2             -      
inter_layer_slice_beta_offset_div2                 -      
