Bitstream file name: TEMPSCAL_B_Panasonic_2.bit
Conformance point:   VTM-9.0
Resolution:          1920x1080
Format:              4:2:0 progressive
Frame rate:          60 frames/second          
Profile:             Main 10 Profile
Tier:                Main Tier
Level:               4.1          

The bitstream was created using the VTM-9.0 encoder with various bug fixes related to DPB and HRD.

Bitstream feature:
The bitstream is for testing temporal scalability with HRD signalling for temporal sublayers.
It has 5 temporal sublayers with a GOP size of 16 and HRD signalling (including buffering period and picture timing SEI message with timing for temporal sublayers). The following encoding structure was used:

GOPSize                       : 16          # GOP Size (number of B slice = GOPSize-1)
#        Type POC QPoffset QPOffsetModelOff QPOffsetModelScale CbQPoffset CrQPoffset QPfactor tcOffsetDiv2 betaOffsetDiv2 CbTcOffsetDiv2 CbBetaOffsetDiv2 CrTcOffsetDiv2 CrBetaOffsetDiv2 temporal_id #ref_pics_active_L0 #ref_pics_L0   reference_pictures_L0 #ref_pics_active_L1 #ref_pics_L1   reference_pictures_L1
Frame1:   B   16   1        0.0                      0.0            0          0          1.0      0            0                0             0                0               0              0             2                3          16 32 24                    2                2           16 32
Frame2:   B    8   1       -4.8848                   0.2061         0          0          1.0      0            0                0             0                0               0              1             2                2          8 16                        2                2           -8 8
Frame3:   B    4   4       -5.7476                   0.2286         0          0          1.0      0            0                0             0                0               0              2             2                2          4 12                        2                2           -4 -12
Frame4:   B    2   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              3             2                2          2 10                        2                3           -2 -6 -14
Frame5:   B    1   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                2          1 -1                        2                4           -1 -3 -7 -15
Frame6:   B    3   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                2          1 3                         2                3           -1 -5 -13
Frame7:   B    6   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              3             2                2          2 6                         2                2           -2 -10
Frame8:   B    5   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                2          1 5                         2                3           -1 -3 -11
Frame9:   B    7   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                3          1 3 7                       2                2           -1 -9
Frame10:  B   12   4       -5.7476                   0.2286         0          0          1.0      0            0                0             0                0               0              2             2                2          4 12                        2                2           -4 4
Frame11:  B   10   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              3             2                2          2 10                        2                2           -2 -6
Frame12:  B    9   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                2          1 9                         2                3           -1 -3 -7
Frame13:  B   11   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                3          1 3 11                      2                2           -1 -5
Frame14:  B   14   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              3             2                3          2 6 14                      2                2           -2 2
Frame15:  B   13   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                3          1 5 13                      2                2           -1 -3
Frame16:  B   15   6       -7.1444                   0.3            0          0          1.0      0            0                0             0                0               0              4             2                4          1 3 7 15                    2                2           -1 1

Bitstream submitter:
Virginie Drugeon
virginie.drugeon@eu.panasonic.com

