== JVT-C151.doc
== New Intra Prediction using Intra-Macroblock Motion Compensation (IMMC)

1. Launch Microsoft VC++ with tml.dsw
2. Batch build the release version of encoder and decoder
3. Go to ./sim. For a simple test of encoder and decoder, "tcsh run.csh"
4. Copy all test sequences into ./sim. Then "tcsh runAll.csh > ../Results/out.txt"

5. Go to ../Results. "tcsh DoGrep.csh out.txt outRaw.txt". The format of outRaw.txt is
	Seq. QP
	Y SNR
	U SNR
	V SNR
	bitrate
	Y SNR
	U SNR
	V SNR
	bitrate
The first set is with IMMC and the second set is without IMMC.

6. Edit outRaw.txt to put the above results in one row for each QP.
7. Load outRaw.txt to Excel properly and save the file to outRaw.xls

8. Calculate the improvement from two RD-curves for each sequence by using curve fitting and integration.

9. A reference of results are included as: JVT-C151.xls, cifRaw.xls and qcifRaw.xls.





