

Annex B NALU w/ long startcode, len 10, forbidden_bit 0, nal_reference_idc 3, nal_unit_type 7

@0      SPS: profile_idc                                      01010000  ( 80)
@8      SPS: constrained_set0_flag                                   0  (  0)
@9      SPS: constrained_set1_flag                                   0  (  0)
@10     SPS: constrained_set2_flag                                   0  (  0)
@11     SPS: constrained_set3_flag                                   0  (  0)
@12     SPS: reserved_zero_4bits                                  0000  (  0)
@16     SPS: level_idc                                        00011110  ( 30)
@24     SPS: seq_parameter_set_id                                    1  (  0)
@25     SPS: chroma_format_idc                                     010  (  1)
@28     SPS: bit_depth_luma_minus8                                   1  (  0)
@29     SPS: bit_depth_chroma_minus8                                 1  (  0)
@30     SPS: lossless_qpprime_y_zero_flag                            0  (  0)
@31     SPS: seq_scaling_matrix_present_flag                         0  (  0)
@32     SPS: log2_max_frame_num_minus4                           00101  (  4)
@37     SPS: pic_order_cnt_type                                      1  (  0)
@38     SPS: log2_max_pic_order_cnt_lsb_minus4                   00101  (  4)
@43     SPS: num_ref_frames                                      00110  (  5)
@48     SPS: gaps_in_frame_num_value_allowed_flag                    0  (  0)
@49     SPS: pic_width_in_mbs_minus1                           0001011  ( 10)
@56     SPS: pic_height_in_map_units_minus1                    0001001  (  8)
@63     SPS: frame_mbs_only_flag                                     1  (  1)
@64     SPS: direct_8x8_inference_flag                               0  (  0)
@65     SPS: frame_cropping_flag                                     0  (  0)
@66     SPS: vui_parameters_present_flag                             0  (  0)


Annex B NALU w/ long startcode, len 4, forbidden_bit 0, nal_reference_idc 3, nal_unit_type 8

@67     PPS: pic_parameter_set_id                                    1  (  0)
@68     PPS: seq_parameter_set_id                                    1  (  0)
@69     PPS: entropy_coding_mode_flag                                0  (  0)
@70     PPS: pic_order_present_flag                                  0  (  0)
@71     PPS: num_slice_groups_minus1                                 1  (  0)
@72     PPS: num_ref_idx_l0_active_minus1                        00101  (  4)
@77     PPS: num_ref_idx_l1_active_minus1                            1  (  0)
@78     PPS: weighted prediction flag                                0  (  0)
@79     PPS: weighted_bipred_idc                                    00  (  0)
@81     PPS: pic_init_qp_minus26                                     1  (  0)
@82     PPS: pic_init_qs_minus26                                     1  (  0)
@83     PPS: chroma_qp_index_offset                                  1  (  0)
@84     PPS: deblocking_filter_control_present_flag                  0  (  0)
@85     PPS: constrained_intra_pred_flag                             0  (  0)
@86     PPS: redundant_pic_cnt_present_flag                          0  (  0)
@87     PPS: transform_8x8_mode_flag                                 1  (  1)
@88     PPS: pic_scaling_matrix_present_flag                         0  (  0)
@89     PPS: second_chroma_qp_index_offset                           1  (  0)


Annex B NALU w/ long startcode, len 14106, forbidden_bit 0, nal_reference_idc 3, nal_unit_type 5

@90     SH: first_mb_in_slice                                        1  (  0)
@91     SH: slice_type                                         0001000  (  7)
@98     SH: pic_parameter_set_id                                     1  (  0)
@99     SH: frame_num                                         00000000  (  0)
@107    SH: idr_pic_id                                               1  (  0)
@108    SH: pic_order_cnt_lsb                                 00000000  (  0)
@116    SH: no_output_of_prior_pics_flag                             0  (  0)
@117    SH: long_term_reference_flag                                 0  (  0)
@118    SH: slice_qp_delta                                     0001101  ( -6)

*********** POC: 0 (I/P) MB: 0 Slice: 0 Type 2 **********
@125    mb_type                                                      1  (  0)
@126    transform size 8x8 flag                                      1  (  1)
@127    intra4x4_pred_mode                                           1  ( -1)
@128    intra4x4_pred_mode                                        0001  (  1)
@132    intra4x4_pred_mode                                           1  ( -1)
@133    intra4x4_pred_mode                                        0001  (  1)
@137    intra_chroma_pred_mode                                       1  (  0)
@138    coded_block_pattern                                    0001101  ( 47)
@145    mb_qp_delta                                                  1  (  0)
@146    Luma # c & tr.1s vlc=0 #c=13 #t1=3             000000000001100  ( 12)
@161    Luma trailing ones sign (0,0)                              000  (  0)
@164    Luma lev (0,0) k=9 vlc=0                                    01  (  1)
