Annex 2 to AVC-598R

List of Tape Demonstrations
(28 October 1993, Daejeon)

No	Organization	Topics	Tape	Doc.	
a	Tektronix	Spatial scalability 
	• Base layer: 0.5 Mbit/s, M=1
	• Enhancement layer: 3.5 Mbit/s, M=3
	• Both layers in 4:2:2	D-60	-	
b	ETRI	HDTV/CTV compatibility	D-60	AVC-534