Bitstream file name: TEMPSCAL_C_Panasonic_3.bit
Conformance point:   VTM-10.0
Resolution:          1920x1080 
Format:              4:2:0 progressive
Frame rate:          60 frames/second          
Profile:             Main 10 Profile
Tier:                Main Tier
Level:               4.1          

The bitstream was created using the VTM-10.0 encoder.

Bitstream feature:
The bitstream is for testing temporal scalability.
It has 3 temporal sublayers with a GOP size of 6. The following encoding structure was used:

GOPSize                       : 6          # GOP Size (number of B slice = GOPSize-1)
#        Type POC QPoffset QPOffsetModelOff QPOffsetModelScale CbQPoffset CrQPoffset QPfactor tcOffsetDiv2 betaOffsetDiv2 CbTcOffsetDiv2 CbBetaOffsetDiv2 CrTcOffsetDiv2 CrBetaOffsetDiv2 temporal_id #ref_pics_active_L0 #ref_pics_L0   reference_pictures_L0 #ref_pics_active_L1 #ref_pics_L1   reference_pictures_L1
Frame1:   P    6   1        0.0                      0.0            0          0          1.0      0            0                0             0                0               0              0             2                2          6 12                        0                0
Frame2:   B    3   1       -4.8848                   0.2061         0          0          1.0      0            0                0             0                0               0              1             2                2          3 9                         2                2           -3 3
Frame3:   B    1   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              2             2                2          1 7                         2                2           -2 -5
Frame4:   B    2   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              2             2                2          2 8                         2                2           -1 -4
Frame5:   B    4   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              2             2                2          1 4                         2                2           -2 10
Frame6:   B    5   5       -5.90                     0.2333         0          0          1.0      0            0                0             0                0               0              2             2                2          2 5                         2                2           -1 11

Bitstream submitter:
Virginie Drugeon
virginie.drugeon@eu.panasonic.com

