Bitfile:       10b444P16_B_Sony_1.bit
Profile:       Main 16 444
Tier:          Main
Level:         4.1
Image size:    1920x1080
Bit depth:     10
Chroma format: 444
Frame rate:    50P
Created by:    VTM14.0
Decoded by:    VTM14.0
Contact:       Adrian Browne (adrian.browne@sony.com)

Content description:
               A random access sequence of 10-bit 444 data encoded in the Main 16 444 profile.
               VVCv2 tools (EPP, ERRC, PRRC, ETSRC, RLSCP) are not used due to bit depth constraint.
