Stream Name:             Hi422FR3_SONY_A
Stream Source:           SONY
Video Sequence:          mobile
Video Resolution:        CIF - 4:2:2  
Video Frames:            5
Frame/Field Coding:      Frame
Entropy Coding:          CAVLC
Slice Types:             IPBPB
I Period:                0
Slices per Picture:      1
Conformance Point:       
POC Type:                0
Number Ref Frames:       0
IDR:                     First only  
Ref Pic List Reorder:    No
Adapt Ref Pic Mark:      Off
Constrained Intra Pred:  Off (Unconstrained)
Weighted Pred (P):       Off
Weighted Bipred (B):     Off
Direct Prediction:       None 
Direct 8x8 Inference:    On
Loop Filter:             Off
SEI:                     No
VUI:                     No
Number Slice Groups:     1
Long-term Ref Frames:    No
MMCO:                    No
Arbitrary Slice Order:   No
Redundant Slices:        No
Gaps in frame_num:       No
Bit Depth Luma:           8
Bit Depth Chroma:         8