Stream Name:  CABAST3_Sony_E 
Stream Source:  Sony  
Video Sequence:  Mobile  
Video Resolution:  CIF  
Video Frames:  300  
Frame/Field Coding:  Frame  
Entropy Coding:  CABAC  
Slice Types:  IPB (multiple slice types per picture)
I Period:  15  
Slices per Picture:  4  
Conformance Point:  JVT-G050r1 (2003/6/02)  

POC Type:  0  
Number Reference Frames:  1  
IDR:  First frame  
Ref Pic List Reordering:  No  
Adaptive Ref Pic Marking Mode:  Off  
Constrained Intra Prediction:  Off (Unconstrained)  
Weighted Prediction (P):  Off  
Weighted Biprediction (B):  Off  
Direct Prediction:  None  
Direct 8x8 Inference:  Off  
Loop Filter:  On  
SEI:  No  
VUI:  No  
Number Slice Groups: 1
Long-term Ref Frames: No
MMCO: No
Arbitrary Slice Order: No
Redundant Slices: No
