Stream Name:  CVMAPAQP3_Sony_E
Stream Source:  Sony  
Video Sequence:  cheer  
Video Resolution:  720x480  
Video Frames:  8
Frame/Field Coding:  Field + Frame  MB AFF
Entropy Coding:  CAVLC  
Slice Types:  IPB  
I Period:  15  
Slices per Picture:  1  
Conformance Point:  JVT-G050r1 (2003/6/02)  

POC Type:  0  
Number Reference Frames:  5
IDR:  First frame  
Ref Pic List Reordering:  No  
Adaptive Ref Pic Marking Mode:  Off  
Constrained Intra Prediction:  Off (Unconstrained)  
Weighted Prediction (P):  Off  
Weighted Biprediction (B):  Off  
Direct Prediction:  None  
Direct 8x8 Inference:  On  
Loop Filter:  On  
SEI:  Yes  
VUI:  No  
Number Slice Groups: 1
Long-term Ref Frames: No
MMCO: No
Arbitrary Slice Order: No
Redundant Slices: No

The QP is changed for each MB based on MB encoding order.
